//          Race Mania modems
//          In this file you will hopefully find your own modem.
//          However if your modem isn't listed or it doesn't respond
//          correctly, you can still enter new commands.
//          When editing this file you should keep in mind that:
//		1.)    First line is a name of your modem.
//             It serves only to distinguish between different
//             modems in setup program.
//      2.)    Second line is an init string. The best thing to do
//			   is to start it with &F which	will reset your modem.
//             Now comes important part: You MUST tell your modem
//             to disable data compression & turn off all error
//             correction.If you've done that then you're almost there.
//      3.)    In third line you enter hangup string. Usually this is
//             AT Z H0.
//      4.)    Forth line is a speed of your modem.
//             To play Race Mania you need 9600bps modem or
//             higher.
//      5.)    Now go to setup program and run modem game. If ERROR is
//             reported then you will have to check your modem init string
//             and try again.


Zoltrix
AT &F X3 &Q6 &K0 %C0
AT Z H0
9600

Intel 14.4i
AT &F \N0 \Q0 \V0 %C0
AT Z H0
9600

SupraFax 14.4 v32
AT &F &Q6 &K %C0 \N1 S37=9
AT Z H0
9600

ZOOM VXP 14.4 v42
AT&F&K0&M0&Q0&D0&C0\G0%C0
AT Z H0
9600

Boca 14.4 fax
AT Z S46=0 S37=9 N0 &Q0 &D2 &K0
AT Z H0
9600

Gateway Telepath 550
ATZS27=32S15=16S13=64&B0&H2&I1&N6&K0&M0
AT Z H0
9600

Boca 14.4 v32 fax
AT \N0 \G0 &K0 %C0 N0 S37=9
AT Z H0
9600

Intel 14.4 fax
AT &F S37=9 N0 &D2 &C1 &Q6 &K0 S0=1
AT Z H0
9600

Digicom Scout Plus 14.4 Fax
AT Z *m0 *e0
AT Z H0
9600

Gateway Telepath 14.4 fax
ATB0N0\N0 %C0 &K0 S37=9
AT Z H0
9600

ZOOM 14.4
AT S37=9 N0 S46=136 %C0 &Q0 \G0
AT Z H0
9600

Intel 14.4i fax
AT&F\N0\Q0
AT Z H0
9600

Practical Peripherials 14.4FX v32
AT Z S46=0 &Q0 &D2
AT Z H0
9600

Hayes Optima 14.4
AT &F S37=9 S46=0 N0 &Q0 &K0
AT Z H0
9600

Cardinal 9600fax
ATZ&Q6&K0%C0\N0N0S37=9
AT Z H0
9600

Generic 14.4
AT &Q6&R1&K0N0 S37=9 \J1 %E1
AT Z H0
9600

GVC 14.4 fax
AT Z S46=0 S37=9 N0 &Q0 &D2 &K0
AT Z H0
9600

GVC 14.4 MNP2-5 v42
AT %C0 \N0 B8
AT Z H0
9600

Intel 14.4 ext
AT\N0/Q0
AT Z H0
9600

SupraFax 14.4 v32-
AT &F S37=9 S46=136 M1 Q0 D2
AT Z H0
9600

Telebit Worldblazer 14.4
AT S51=4 S180=0 S183=8 S190=0 L1
ATH
14400

USRobotics 14.4 v32 fax
AT &F &M0 &I0 &K0 B0 &N6
AT Z H0
9600

ZOOM VFX v32
AT &K0 &Q0 &D2 E1 V1 X4 N0 &Q0 S37=9
AT Z H0
9600

ZOOM 14.4 v32 v42 fax
AT &F S37=9 N0 &D2 &C1 &Q6 &K0 S0=1
AT Z H0
9600

MegaHertz C596FM
AT &F \N1 \J0 &Q0 %C0
AT Z H0
9600

Smart One 1442F
AT Z %C0 &Q0 &K0 &D2 S37=9 S95=44 S46=0
AT Z H0
9600

Viva 14.4i fax
AT\N0\Q0\J1\VI
AT Z H0
9600

SupraFax 14.4 v32
AT &F0 S46=136 %C0
AT Z H0
9600

Infotel 14.4
AT &Q6 %C0 S37=9 N0 &K0
AT Z H0
9600

Zoomfax VFP v32
AT &Q0 S48=128 S36=1 S37=9 N0 S46=136 &D2
AT Z H0
9600

ZyXEL U-1496 14.4
AT Z S46=0 &D2 &K0
AT Z H0
9600

Identity Internal
AT &F0 B8 %C0 \Q0 \N1
AT Z H0
9600

GENERIC 9600
AT &F1 &K0 &M0 &Q0 &D2 S46=0
AT Z H0
9600

VivaFax 14.4
AT\Q0 &M0 %C0 B8 \N1
AT Z H0
9600

VivaFax 14.4
AT &F &C1 &D2 N0 \N1 %C0 &K0 S37=9
AT Z H0
9600

GENERIC
AT &B0 &K0 &Q0 &D0 &C0
AT Z H0
9600

USRobotics 14.4 fax
AT S0=1 S7=60 E1 Q0 V1 &C1 &D2 &K0 &N6 &A3
AT Z H0
9600

ZOOM VFP 14.4
AT &K0&Q0&D2E1V1X4S37=9N0
AT Z H0
9600

Telepath 550
AT Z &N6 &M0 &K0 S0=1
AT Z H0
9600

USRobotics Sportster 14.4
AT Z &K0 &M0 &D2 E1 V1 X4
AT Z H0
9600

Hayes Optima 14.4
AT Z\N0
AT Z H0
9600

Viva 14.4
AT Z\N0
AT Z H0
9600

ZyXel 14.4
AT Z\N0
AT Z H0
9600

Hayes Ultra 14.4
AT &F &C1 &D2 &Q &K
AT Z H0
9600

Cardinal 14.4 v32
AT&F&Q0N0S37=9
AT Z H0
9600

Acubit 14.4 fax v32
AT Z S37=9 %C0 \N1
AT Z H0
9600

AT&T Data Port 14.4 FaxM.
ATZ S41=3 %B9600 \N0 %C0
AT Z H0
9600

Redicard v.32 bis 14.4
AT %C & \N
AT Z H0
9600

USR Sportster 14.4 v32 fax
AT &F &M0 &I0 &K0 B0 &N6
AT Z H0
9600

// Sorry, but there are no more modems listed.
// If you cannot find your modem in the list,please enter your own
// modem strings. It's easy when(if) you know how...
