PLATFORM TYPE:   TR-1700 DIESEL ELECTRIC SUBMARINE
PLATFORM NAME:   SAN JUAN (S 42)
                 SANTA FE (S 44)

DESCRIPTION:     HUNTER KILLER SUBMARINE
SPEED:           15KTS SURFACED
                 25KTS DIVED
MANNING:         26
DIMENSIONS:      217 x 24 x 22 FT
DISPLACEMENT:    2,264
RANGE:           10425NM 8KTS SURFACED
                 460NM AT 6KTS DIVED
POWER PLANT:     4 DIESEL ELECTRIC MOTORS 9,000 SHP
                 1 SHAFT

RADAR:
    (SURFACE SRCH):    PERISCOPIC
    (FIRE CONTROL):    SIGNAL SINBADS

ELECTRONIC WARFARE:
    (ESM):             RWR

SONAR:           KRUPP ATLAS ACTIVE/PASSIVE

COUNTRIES:       GERMANY; BUILT UNDER CONTRACT FOR
                 ARGENTINA IN 1977
