PLATFORM TYPE:   HEROJ CLASS PARTOL SUBMARINE
PLATFORM NAME:   HEROJ 821

DESCRIPTION:     BASED ON SOVIET SUBMARINE DESIGN AND
                 USES SOVIET-MADE ELECTRONICS AND
                 ARMAMENT
DISPLACEMENT:    960 DIVED
DIMENSIONS:      182.7 x 23.6 x 16.7 FT
POWERPLANT:      2 DIESELS, DIESEL-ELECTRIC, 1600HP
                 2 GENERATORS
                 1 MOTOR, 1560 HP
                 1 SHAFT
SPEED:           10KTS SURFACED
                 16KTS DIVED
MANNING LEVEL:   27

TORPEDOES:       6  21 IN (533mm) BOW TUBES
                 10 SOVIET TYPE 53
                 10 SWEDISH TP 61

COUNTERMEASURES:
    (ESM):       STOP LIGHT, RADAR WARNING

RADARS:
    (SURFACE SRCH):     SNOOP GROUP (I-BAND)

COUNTRIES:              YUGOSLAVIA
COMMENTS:               DIVING DEPTH 980 FT.

 
