SUBMARINE TYPE:  TYPHOON CLASS SSBN

SPEED:           26 DIVED
MANNING LEVEL:   200
DIMENSIONS:      562.7 x 80.7 x 42.7 FT
DISPLACEMENT:    21,500 SURFACED
                 26,500 DIVED
POWERPLANT:      2 NUCLEAR TURBINES 81,600 HP
                 2 SHAFTS
                 SHROUDED PROPS

SURFACE-TO-SURFACE MISSILES:
                 20 SS-N-20 STRUGEON

SURFACE-TO-AIR MISSILES:
                 MAY HAVE SAM CAPABILITY

TORPEDOES:       2  21 IN (533mm) TUBES 
                 4  25.6 IN (650mm) TUBES 
                 36 TORPEDOES AND A/S MISSILES

RADARS:
    (SURFACE SRCH):    SNOOP PAIR (I/J-BAND)
    (IFF):             KREMMY 2

COUNTERMEASURES:
    (ESM):             RIM HAT RADAR W ARNING
                       PARK LAMP (D/F-BAND)

SONARS:                SHARK GILL HULL-MOUNTED
                       PASSIVE/ACTIVE SEARCH AND ATTACK
                       HIGH FREQUENCY
                       MOUSE ROAR HULL-MOUNTED
                       ACTIVE ATTACK, HIGH FREQUENCY

SATCOM:                PERT SPRING

COUNTRIES:            CIS
COMMENTS:             THIS IS THE LARGEST TYPE OF
                      SUBMARINE EVER BUILT

 
