MISSILE NAME:    SA-2 GUIDELINE
FUNCTION:        MEDIUM-RANGE SURFACE-TO-AIR TACTICAL
                 GUIDED MISSILE
GUIDANCE:        RADIO COMMAND
RANGE:           27NM
SPEED:           2243.5KTS
ALTITUDE:        54,000 FT

COUNTRY:         CIS AND EXPORTED TO VARIOUS OTHER
                 COUNTRIES
COMMENTS:        MISSILE MUST BE GATHERED TO THE RADAR
                 BEAM IN THE FIRST SIX SECONDS OF
		 FLIGHT OR IT WILL NOT BE ACQUIRED
                 AT ALL
