PLATFORM TYPE:   OSA I CLASS GUIDED MISSILE BOATS

DESCRIPTION:     SMALL MISSILE CORVETTE DESIGNED FOR
                 ANTI-SHIPPING OPERATIONS
SPEED:           36KTS
RANGE:           500 AT 34KTS
                 750 AT 25KTS
MANNING LEVEL:   30
DIMENSIONS:      126 x 25 x 6 FT
DISPLACEMENT:    215 FULL LOAD
POWERPLANT:      3 DIESEL ENGINES 12,000 HP
                 3 SHAFTS

GUNS:            4  30mm (2 TWIN)

SURFACE-TO-SURFACE MISSILES:
                 4 SS-N-2A/B STYX ANTI-SHIP (4 SINGLE)

SURFACE-TO-AIR MISSILES:
                 1 SA-N-5 ANTI-AIR LAUNCHER
                 1 SA-N-8 ANTI-AIR LAUNCHER

RADARS:
    (SURACE SRCH/TARGETING):
                 1 SQUARE TIE
    (FIRE CTRL): 1 DRUM TILT

COUNTRY:         CIS AND EXPORTED TO VARIOUS OTHERS.
COMMENTS:        STEEL-HULL MISSILE BOATS, DEVELOPED
                 TO SUCCEED THE WOOD-HULL KOMAR CLASS
                 SHIPS.


 
