:WELCOME
 Welcome to POWERLan's Install Program
  Here are a few tips to get your network up and running quickly:

   Be sure your network adapter cards are properly installed.

   Decide which machines will be workstations and which will be servers.
    A server can share its disk resources with other machines on the
    network. While a workstation cannot share its disks, it can access
    those of a server. FOR QUICK SETUP, INSTALL A SERVER FIRST.

   Printers can be shared from servers OR workstations. Designate ONE
    server to act as the "spool server" for the network. FOR QUICK
    SETUP, attach your shared printer(s) to the spool server. OR,
    add at the spool server a "print profile" with the printer name.

   During install, respond Yes to share all drives at all servers.
    Sharing drives is just the first step for users to access them.
    Use PLADMIN to assign redirections (USEs) to those shared disks.

   The user named as the administrator is automatically "created"
    during install. Use PLADMIN to create all other users named during
    install (or later) before those users can log on to the network.

   At the end of install, you will be able to change your responses.
:PNWELCOME
 Welcome to POWERLan's Install Program
  Here are a few tips to get your network up and running quickly:

   Be sure your network adapter cards are properly installed.

   Decide which machines will be workstations and which will be servers.
    A server can share its disk resources with other machines on the
    network. While a workstation cannot share its disks, it can access
    those of a server. For quick setup, INSTALL A SERVER FIRST.

   During install, printers can be shared only from servers. To share
    a printer from a workstation after install, consult documentation.
    To access a printer, assign a USE for LPTn to the printer name.

   During install, respond Yes to share all drives at all servers.
    Sharing drives is just the first step for users to access them.
    Use PLADMIN to assign redirections (USEs) to those shared disks.

   Any user named during server install is automatically created. You
    must use PLADMIN to create users named during workstation install.
    For quick setup, create all WORKSTATION users when you install the
    first server, and then continue installing other machines.

   At the end of install, you will be able to change your responses.
:FROM
You probably won't need to modify this field.  It contains the 
directory from which files will be copied.  Press <tab> to move on 
to the next field.
:TO
This field contains the directory to which POWERLan will be installed.
You probably won't need to modify this field.  It defaults to C:\PL.
If you don't want to install to your C drive, or if you want to change
the name of the POWERLan directory, you can edit this field.
:MACHINETYPE
This machine can be either a workstation or a server.  If you don't want
to share this machine's disks, select Workstation.  Note that POWERLan
allows both workstations and servers to share printers.
:BOARDTYPE
Press the <space bar> to display a list of board types.  Select the type 
of network interface card being used in this machine.
:BEGIN
Before starting the installation, you should make sure you have made any
desired modifications to the above fields.  Press <Enter> to start the 
POWERLan installation.  
:CANCEL
Press <Enter> to exit without installing POWERLan.  By exiting without 
installing, no directories will be created on your disk, and no POWERLan
files will be copied.
:DOSONLY
To perform a full DOS and Windows installation of POWERLan, press 'N'.
This will exit this program and leave instructions on the screen for
installing under Windows.  If you don't use Windows and want to perform 
the DOS only installation of POWERLan, press 'Y'.
