=================================================================
README.ARS                                               11/12/92
=================================================================

This README file contains information about the sound card
drivers currently available with WP Presentations.  Sound cards
are listed below, along with the name of the .ARS file and .COM
file(s) that are designed to support them.  Each sound card
requires an .ARS file and two or more .COM files.  Each sound
card requires VMP.COM, in addition to the .COM file written
specifically for that card.  For example, if you have a
SoundBlaster Pro, you would need TAPISB.COM, and VMP.COM.

Before selecting a sound card, make sure the .ARS and .COM files
have been installed into the same directory where you installed
WP Presentations.  The WP Presentations program will find the
files and automatically display the menu choices associated with
the driver in the Sound Card Type dialog box.

Any .ARS and .COM files that do not pertain to your hardware can
be deleted to free up disk space.  However, VMP.COM should not be
deleted, as it is necessary for the other .COM files to run.


LOADING SOUND DRIVERS INTO HIGH MEMORY
=================================================================
If you need more memory to run WP Presentations, you can load the
sound drivers into high memory using a memory manager.  These
drivers must be loaded into high memory before starting WP
Presentations.  For more information on loading sound drivers
into high memory, see your memory manager manual.

When loading, begin by loading the specific driver for your card,
then load VMP.COM.  For example, if you have a SoundBlaster Pro
card, you would first load TAPISB.COM, then VMP.COM.  Note: If
you are using the Adlib PC Game Card, you must load the following
drivers in this order: VAPINUL.COM, SAPIFM1.COM, VMP.COM. 

WordPerfect Presentations will recognize that the drivers have
been loaded and will not try to load them again.


SELECTING A SOUND CARD
=================================================================
To select a sound card,

1    Choose Setup from the file menu, then choose Slide Show.

2    Choose Sound Card Type.

3    Highlight the correct sound device, then choose Select.


Sound Card                         .ARS File         .COM File(s)
=================================================================
Adlib PC Game Card                 FM1.ARS           VAPINUL.COM
                                                     SAPIFM1.COM
ATI AudioFX                        ATI.ARS           TAPIATI.COM

ATI StereoFX                       ATI.ARS           TAPIATI.COM

CompuAdd                           CUA.ARS           TAPICUA.COM

IBM PS/1                           PS1.ARS           TAPIPS1.COM

MediaVision Spectrum               MV.ARS            TAPIMV.COM

MediaVision Spectrum-16            MV2.ARS           TAPIMV2.COM

MediaVision Spectrum-Plus          MV2.ARS           TAPIMV2.COM

MusicQuest 16s                     V16.ARS           VAPI16S.COM

MusicQuest MQX-32                  MQX.ARS           VAPIMQX.COM

PC Internal Speaker                STANDARD.ARS      *

Roland LAPC-1                      MPU.ARS           VAPIMPU.COM

Roland MPU 401                     MPU.ARS           VAPIMPU.COM

SoundBlaster                       SB.ARS            TAPISB.COM

SoundBlaster Pro                   SB.ARS            TAPISB.COM

Voyetra V-22                       V22.ARS           VAPI22.COM

Voyetra V-24s                      V24.ARS           VAPI24S.COM

Yamaha TG100                       TG.ARS            VAPITG.COM


*    PC Internal Speaker does not require a .COM file.