May 1, 1995 (c) Copyright 1994 Palindrome Corporation. All
rights reserved.
			  PALSHELL.TXT

PALSHELL.NLM allows you to perform operations at the server console 
that you would normally perform from the Windows interface.

SYNTAX
The syntax for PALSHELL.NLM is:

LOAD PALSHELL.NLM /OP=<operation code> [options]

BACKUP OPERATIONS
=================

Operation                                         Code
---------                                         ----
Automatic Backup                                  CC 
Archive Resource                                  AA
Archive Files (list)                              AL
Backup Files (list)                               BL
Full Backup (Resource)                            BF
Incremental Backup                                BI
Differential Backup                               BD
Migrate Resource                                  MA
Migrate Files (list)                              ML
Database Maintenance                              DM
Database Verification                             DV 

Options                                           Code
-------                                           ----
Clear Archive Bit                                 /B=Y
Do Not Clear Archive Bit                          /B=N
File List                                         /C<name of file>
Include File                                      /F+<file spec>
Wildcard files to include                         /FW+<file spec>
Exclude File                                      /F-<file spec>
Media to use (Label)                              /L<name>

Managed Media (options)
Copy fully protected files already in set         /MM=YY 
Copy fully protected not already in set           /MM=YN 
Copy files not fully protected already in set     /MM=NY
Copy files not fully protected, not in set        /MM=NN

Non-Managed Media (options)
Append and track backup session                   /MN=AT
Append and do not track backup session            /MN=AX
Erase sessions and track backup session           /MN=ET
Erase sessions and do not track backup session    /MN=EX

Perform backup in Unattended mode                 /Q
Source name space                                 /SN<name space> 
Logical Device name                               /U<device name> 
Verify sessions                                   /V
Calculate and Verify sessions                     /VC
Verification off                                  /VN
SCSI Device Trace                                 /W 

Backup Operation Examples
=========================
Perform Automatic Backup
     LOAD PALSHELL   /OP=CC  /Q                
     (backs up entire Protected Resource List in unattended mode)

Full Backup of Resource
     LOAD PALSHELL   /OP=BF  FS1\SYS:  /Q
     (backs up FS1\SYS: in unattended mode)
						  
 
    
RESTORE OPERATIONS
==================

Operation                                         Code
---------                                         ----
Restore Full Resource                             RRA
Restore All Files on Resource                     RRF
Restore the System Control Database               RC
Restore a File History Database                   RH
Restore files to original location                RO
Restore directory structure of resource           RD
Restore files without restoring directories       RF
Restore and redirect files                        RR

Option                                            Code
------                                            ----
Files to include                                  /F+<file spec> 
Wildcard files to include                         /FW+<file spec>
Files to exclude                                  /F-<file spec>
Media to use (Label)                              /L<name>
Never overwrite files on collision                /PN
Always overwrite files on collision               /PA
Prompt on overwrite if file collision             /PP
Overwrite files if file on disk is older          /PO
Name space of target resource is DOS              /RNDOS 
Name space of target resource is AFP              /RNAFP
Name space of target resource is NFS              /RNNFS
Target Resource (e.g. FS1\SYS:)                   /RR<resource>  
Target path                                       /RP<path>
Perform restore in Unattended mode                /Q
Source name space                                 /SN<name space>
Logical Device name                               /U<device name> 
Verify sessions                                   /V
Verification off                                  /VN
SCSI Device Trace                                 /W 

Restore Operation Examples
==========================

Perform Full Resource Restore:
LOAD PALSHELL   /OP=RRA  FS1\SYS: /Q
(restores FS1\SYS: in unattended mode)

Restore file to original location:
LOAD PALSHELL /OP=RO   FS1\SYS:  /F+\TEST.FIL
(restores TEST.FIL to the root of FS1\SYS:)
 

UTILITY OPERATION CODES
=======================

Operation                                         Code
---------                                         ----
Copy Media                                        MC
Journal Media                                     MJ
Format Media                                      MF
Retension Media                                   MT
Secure Erase Media                                MS
Verify Media                                      MV
Short Test on Device                              DST
Long Test on Device                               DLT
Media Changer Test (autoloaders only)             DMT
Autoloader unload request                         LU
Autoloader load request                           LL 
Autoloader export request                         LE 
Autoloader import request                         LI

Option                                            Code
------                                            ----
Session Name                                      /D<name>   
Media to use (Label)                              /L<name>
Perform utility operation in Unattended mode      /Q
Target Device Name                                /TD<name>
Logical Device Name                               /U<device> 
Verify sessions                                   /V 
SCSI Device Trace                                 /W 

Utility Operation Examples
==========================
Format specific media
LOAD PALSHELL /OP=MF /LADMIN:A:1   /Q

Copy media
LOAD PALSHELL /OP=CM  /UTAPEDRIVE /TDOPTICAL_DRIVE  /Q
(where TAPEDRIVE is the source device containing the media to be
copied and OPTICAL_DRIVE contains the target media)


Translate History Database                   /XH  /N<volume ame>

LOAD PALSHELL /OP=XH  /NFS1\SYS:
(translates FS1\SYS: File History Database)
