This disk contains medium changer device driver files
for Backup Exec for Windows NT.  This disk's root
directory has three subdirectories, "i386", "mips",
and "alpha, for the Intel (i386), Mips, and Alpha
versions of Windows NT. Each contains the "scsichng.sys",
device driver file for the corresponding version of
Windows NT.

Use Windows NT Setup to install the medium changer device
driver:

1) Double click on the "Windows NT Setup" icon in the "Main"
   program group.

2) Select "Add/Remove Tape Devices..." in the "Options" menu
   of Windows NT Setup.

3) Select "Add.." in the "Tape Device Setup" window.

4) Open/expand the "Device:" list in the "Select Tape Device
   Option" window.

5) Select "Other (Requires a disk from a hardware manufacturer)"
   at the bottom of the "Device:" list in the "Select Tape
   Device Option" window.

6) Enter the drive/path to the appropriate files on this disk
   in the "Insert Diskette" window; e.g., "a:\i386" for the
   files for the Intel (i386) version of Windows NT, "a:\mips"
   for the files for the Mips version of Windows NT, and
   "a:\alpha" for the files for the Alpha version of Windows NT.

7) Select "OK" in the "Insert Diskette" window.

8) Select the line in the "Choose a Tape Driver supported by
   this hardware manufacturer's disk." list in the "Select
   OEM Option" window; i.e., select the medium changer driver.

9) Select "OK" in the "Select OEM Option" window.

10) Select "Install" in the "Select Tape Device Option" window.

11) If it appears, then select "New" in the "Windows NT Setup"
    window; otherwise, enter the same drive/path to the
    appropriate files on this disk that was used in step #6
    above.

12) Select "Continue" in the "Windows NT Setup" window.

The "Tape Device Setup" window will re-appear with the medium
changer selected in step #8 now included in the "Tape Devices
installed on ..." list. Close the "Tape Device Setup" window,
close/exit Windows NT Setup, and restart Windows NT to
activate the changes made.


-------------------------------------------------------------

The following is a list of Medium Changers which are supported
by Backup Exec for Windows NT.

Medium Changers
---------------

ADIC 4mm DAT Autochanger
ADIC VLS 8mm DAT Loader
Compaq 4586 Loader
Conner Diamondback Loader
Conner 5L-DLT
Conner 7L-DLT
DEC TLZ6 Loader
DEC\Cipher L860 (L7A) Loader
DEC DLT 2500 Loader
Dilog Libra Loader
Exabyte 10e Loader
Exabyte 10i Loader
Exabyte 210 Loader
HP 1553A Loader
HP SureStore 1200E
IBM 4586 DiamondBack
Lago LS/380 DataWheeel
SpectraLogic Spectra4000


NOTE:  All trademarks and registered trademarks are property
of their respective owners.

