                        Gammalink
                        1314 Chesapeake Terrace
                        Sunnyvale, CA. 94089
                        Voice:  408-744-1400
                        FAX:    408-744-1900



        This file contains inportant information that should be read BEFORE
installation of the GammaFax Software is done.  This file contains the most
up-to-date information about the software including any known bugs.


==============================================================================

        GammaFax 5.3.5 Software Installation Notes



Truncation of directory names
=============================

The GammaFax Software installation uses the standard DOS directory and file-
naming conventions.  This specifies that files and directories must follow
the "8.3" file-name standard.

A directory name of more than 8 characters will be trunctated to 8 characters
(i.e \FAX12345678 will be trunctated to \FAX12345).  No warning or error
messages will be generated.


Installation source drive
=========================

The GammaFax Software installation requires the source drive be the logged drive
when INSTALL.EXE is executed.  If you are installing from A:, do the following:

>A:
>install


Strings containing spaces
====================================

The GammaFax Software installation program will ask for the following pieces of
information during the installation procedure:

1.  CSID
2   User name or company name
3.  voice and fax phone numbers

each of the above pieces of information is represented as a string.  To include
spaces within the string (such as between first and last name), you must put
quotation marks around the string.  For example, when entering the name
Joe Smith, it would be entered as "Joe Smith".

==============================================================================

        GammaFax 5.3 Software Post-Installation Instructions


GFSETUP Utility
===============

GFSETUP is a utility that can be used to configure the GammaFax Software
after installation has already been done.  It will configuration of
the following components of the GammaFax system:

1. Individual fax channels (country codes, CSID, etc.)
2. Printer used to print faxes that are received
3. Display type used to display faxes
4. Cover Page information


Please see the GammaFax Reference Manual for further information about this
utility.



FAXM configuration
==================

A.  CSID


The FAXM utility has it's default CSID set to "YOUR CSID".  If you plan
to send faxes using FAXM, you need to change this value to match the value
that is set in your GFAX.$DC configuration file.  To do this follow these
steps:


1.  Start FAXM (or FAXM2P if using OS/2).
2.  Go to the SETUP -> Communication menu
3.  Use the down arrow key to move down to the entry called
    "Your Fax Phone Number . . . (CSID)".
4.  Type in your Fax phone number
5.  Press the ENTER key three times
6.  Hit the S key to save the change.




==============================================================================
                       Do You Need Technical Support?

        GammaFax users who need technical support should submit the
   following information via GammaFax or a fax machine to the Technical
   Support fax machine at +1-408-745-2390.
        Please provide ALL information requested below.  Forms
   submitted incorrectly will take longer to process.

   (1)  Your name and company
   (2)  Voice phone number
   (3)  Fax machine phone number (if you have one)
   (4)  GammaFax phone number
   (5)  Contents of AUTOEXEC.BAT, CONFIG.SYS, and GFAX.$DC
   (6)  A directory listing of the files in the fax directory
   (7)  Name of computer system and type of microprocessor
   (8)  Operating system type and version
   (9)  GammaFax software version
   (10) GammaFax board serial number (located on the board)
   (11) Listing of ALL boards in the computer (*)
   (12) Are you running a network?  If yes, who makes it?
        a) Novell (full version number)
           3Com 3Plus or 3Plus Open
           PC-LAN
        b) Type and brand of network card?
   (13) Do you have a scanner?  What are the name brand and model type?
   (14) Do you have a printer?  What are the name brand and model type?
   (15) Name of display monitor and display card
   (16) Please explain the exact problem in full detail.  Problems
        that are not explained in full or are not understandable will
        take longer to solve, so please be explicit.

   (*)  It is absolutely essential that ALL boards be given.  If
        possible, try also to get the I/O addresses and interrupt
        levels of these boards.

   Please fax us this information at +1-408-745-2390.  We will respond
   to your problem as soon as possible.


===============================================================================

                  GAMMAFAX SUGGESTION AND BUG REPORT

        We welcome any suggestions for improvements and reports on
   problems you may be having.  Please fill out this form and fax or
   mail it to GammaLink.

   GammaLink
   1314 Chesapeake Terrace
   Sunnyvale, CA 94089
   Fax:   +1-408-745-2390   ATTEN:  Technical Support
   Voice: +1-408-745-2250
   CompuServe:  75300,2226
   Internet:  techs@gammalink.com


   NAME: _______________________________ COMPANY: __________________________

   DEPARTMENT: ______________________________ TITLE: _______________________

   ADDRESS: ________________________________________________________________

   CITY: _____________________________ STATE: ______ ZIP: __________________

   YOUR VOICE NUMBER: _____-_____-_______    FAX NUMBER: _____-_____-_______

   DATE PURCHASED: __/__/__ WHERE PURCHASED: _______________________________

   PRIMARY USE OF GAMMAFAX: ________________________________________________

   GAMMAFAX REVISION NUMBER: ___._____ GAMMAFAX SERIAL NUMBER ______________

   TYPE OF COMPUTER: ____________ TYPE OF MONITOR AND CARD: ________________

   OPERATING SYSTEM:   DOS   OS/2   UNIX    REVISION: _______________

   TYPE AND BRAND OF NETWORK_________________________________________

   TYPE AND KIND OF NETWORK ADAPTER__________________________________

   OTHER CARDS IN SYSTEM: __________________________________________________

   _________________________________________________________________________

   DESCRIBE THE PROBLEM IN FULL, INCLUDING HOW TO RECREATE THE FAILURES.
   ALSO ATTACH COPIES OF THE CONFIG.SYS, AUTOEXEC.BAT AND GFAX.$DC FILES.
   PLEASE INCLUDE A LISTING OF THE FILES IN THE FAX DIRECTORY.
     GammaLink Registration Card
     Please complete and return this sheet to GammaLink.   Use
     any word processor to fill it out.

     Name:
     Title:                                  Dept.:
     Company:
     Address:
     City/State/Zip:
     Phone:                                  Fax:


====================================================================

        F.R.E.D (Fax Retrieval of Electronic Documents)



GammaLink offers a service where you can have easy access to GammaFax data
sheets, newsletters, technical tips, and more.  Call 408-734-9906 with your
touch tone phone and request document #100 for an index of all available
documents.  The listings are updated frequently to ensure that our valued
customers are kept abreast of the latest product, pricing, and technical
bulletins.
