           =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

                         Adaptec Easy CD Creator 3.0

                    (c) Copyright Adaptec, Inc. 1995-1997

           =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
Welcome to Adaptec Easy CD Creator
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

The following information is available in this README file:


  o  UNINSTALLATION
  o  WINDOWS 95/NT GENERAL TROUBLESHOOTING


=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
INSTALLATION AND UNINSTALLATION
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

  To Uninstall in Windows 95 or NT 4.0:

     Use the standard uninstall feature "Add/Remove Programs" in the
     Control Panel.


=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
WINDOWS 95/NT GENERAL TROUBLESHOOTING
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

  o  The Teac CD-R50S CD-R drive (4x write) and the Pinnacle RCD 4x4 (4x
     write) only work with certain brands of CD-R media.  If you encounter
     problems creating discs using Easy CD Creator with these drives, you can
     try slowing the write speed from 4x to 2x.  Please consult your drive
     documentation for the supported media list.

  o  The Teac CD-R50S CD-R drive (4x write) and the Pinnacle RCD 4x4 (4x
     write) do not support mixed mode Disc at Once (DAO).

  o  Some CD-R/CD-RW drives will only extract audio at 1x.

  o  If you select "Cancel" when doing a test run of a Disc at Once disc,
     Easy CD Creator may not return control to you right away.  A few drives
     exhibit this problem since they don't return control to Easy CD Creator
     in a timely manner.

  o  Not all CD-ROM drives support digital audio extraction.  Easy CD Creator
     will notify you if it cannot extract audio from your CD-ROM drive.  In
     this case, we recommend you use your CD-R/CD-RW drive to extract audio.

  o  If you are copying CDs or audio tracks from a source ATAPI CD-ROM
     drive, you may experience buffer underruns if your CD-ROM drive is
     not fast enough to keep up with your CD-R/CD-RW drive.  If you
     experience this, you should try reducing your write speed to 1x, or
     buffer to your hard drive first.

  o  We currently do not support ATAPI changers as the source drive for
     CD copying or digital audio extraction.  This limitation does not
     exist for SCSI CD Changers.

