Winsock v2.2 for Windows 95/98 plus fixes (c) Microsoft

Fix: winnuke, jolt, ssping, teardrop & land

Installation:

Windows 95:

Run these programs in the following order:

Step 1: wsockupd.exe - Update Winsock - Reboot
Step 2: msdun12.exe - Update to DialUp Networking 1.2 - Reboot
Step 3: wsock2setup.exe - Winsock 2.2 Upgrade - Reboot
Step 4: vipup20.exe - Winsock 2.2 Patch (Jolt,Ssping,TearDrop) - Reboot
Step 5: vtcpup20.exe - Land Patch for Winsock 2 - Reboot

It is important to do them in this order and also important you go
through each reboot process (even when it doesn't ask to reboot,
reboot! Reboot between EACH process (msdun12.exe will reboot you
twice)).

Windows 98:

If you're running Windows 98, you only need to do steps 4 & 5.
Windows 98 already comes with Winsock v2.2, and DialUp 1.2.

