    ______________________
  z$$$$$$$$$$$$$$$$$$$$$$$        _____________________________________________
 J$`        ___         4$      z$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
 $F   ______$$$______   4$     J$`  Radium presents                          4$
 $F  |$$$$$$$$$$$$$$$p  4$_____$F                                            4$
 $F   ŻŻŻŻŻŻŻŻŻŻŻŻ)$$$  4$$$$$$$F   Point CD audio 32bit v2.3                4$
 $F  |$$$$$$$$$$$$$$U'  4$     $F   (c) Point Software and Systems           4$
 $F  |$$F    d$         4$     '$b                                          d$'
 $F  |$$F   '$$$.       4$       '$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$'  
 $F  |$$F    '$$$$.     4$            ||                                       
 $F  $$$       "$$$$ż¸  4$        ____||_______________________________________
 $F   ŻŻ         ŻŻŻŻŻ  4$      z$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
 $k   r  a  d  i  u  m  $$     J$`  Cracker    : Freeform                    4$
 '$b                   d$'     $F   Supplier   : CDR400 and jazzmaster       4$
   '$$$$$$$$$$$$$$$$$$$'       $F   packaging  : Sandor                      4$
                               $F   prog type  : Red Book Audio CD Writing   4$
                               $F   released   : March 7, 1998               4$
                               '$b  disks      : 1 x 1.05 Mb                d$'
                                 '$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$'

                                                                    ||
   _____              ______________________________________________||_________
 z$$$$$$ Release.info $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
J$`                                                                          4$
$F  PoINT CDaudio 32 is an application to write Red Book Compatible audio    4$
$F  cds. Assembly of the wave files, tracks and idexes is handled by Sek'd   4$
$F  Samplitude Studio, which then sends the TOC to Point CD 32 for burning.  4$
$F  See the end of this nfo for a list of supported drives. (RETAIL $450)    4$
$F                                                                           4$
$F  Whats new from version 2.2 >> version 2.3 :                              4$
$F  Support for NOMAI 680RW, JVC XR-W2040, KodakPCD240,KodakPCD Writer 660,  4$
$F  Matsushita CW-7502, Olympus CDS620E,Philips CDD3610,Pioneer DR-R504X,    4$
$F  and Sony CDU928. Interface and printing support has also been improved.  4$
$F                                                                           4$
$F  Opinion : We spent a week testing this one, and a few of the testers     4$
$F  said they thought this program was harder to learn than CD Architect     4$
$F  from SonicFoundry. This program has gained a following though (Point is  4$
$F  one half of the well known 'Red Roaster' package) and many people will   4$
$F  want to use version 2.3 for its updated drivers and 32 bit update. To    4$
$F  make it easy, |nterfind has written a tutorial that walks you through    4$
$F  burning a cd to hopefully make things easier for new users. A Special    4$
$F  thanks to Deepzone, Hsemzk, Freeform, Finsitez, CDR400, and |nterfind!   4$
'$b                                                                         d$'
  '$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$Radium97$$$$$$$$$$'


Installing PointCD Audio 32 v2.3 :
1) run 'pcdsetup.exe' to install
2) The install will ask for your master disk. You can either copy the included
   "UID.dat" to a floppy, or enter the dir where uid.dat is on your harddrive.
3) Enter ANY name and company.

You will need to be sure to have Sampltude Studio v4.05 installed, since 
Point needs samplitude to build the TOC files.


TUTORIAL : HOW TO CREATE AN AUDIO CD
------------------------------------
1) Start Samplitude Master or Samplitude Studio
2) Create a new multitrack project (type -e- on your keyboard)
   Select 'Stereo 2 Tracks (CD TOC)'. Make sure you save your new *.vip file
   to a dirname with no spaces in it!
3) Open Menu 'File > Load Audio CD Track(s)'
4) Insert your favorite Music CD in your CD Drive
5) Press the 'Track List Copy Play' button and select the tracks you want
6) Now press the button 'Copy selected Track(s)'
7) Enter a Filename for your Wav files. **These also must be saved
   to a dir name that doesnt have spaces in them **
8) Now your VIP-Project includes your CD-Tracks and automaticly adds
   index to all Tracks
9) Open Menu 'Tools > CD > Make CD (no calculations)' to generate a TOC-File.
   if you get an error that it can open a file, you need to resave your
   project withou spaces in it.

10) Start CDaudio32
11) Open Menu 'File > Open' and select your xxx.toc File.
    Find it in the same dir you copied the wave files.
12) Open Menu 'File  > Write to CD-R'
13) Select the Recording Speed and press [Write]

Note : If you have problems loading a TOC into point, it is most likely
because of a space you have put in a filename or directory name.


   ____________________________________________________            __________
 z$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$ Group.news $$$$$$$$$$$
J$`                                                                          4$
$F  Welcome to RickyJ!!  Oh, be sure to check out Sharon-X's new song        4$
$F  titled 'Radium-info' (http://blue.org/Analog_Pussy)  Someone sign this   4$
$F  girl now. Shes got talent. :)                                            4$
$F                                                                           4$
$F  People we are looking for in Radium :                                    4$
$F  * t3 siteops or good Topsite HQ affils                                   4$
$F  * Software suppliers  (Meaning people that work at music stores, at      4$
$F    review magazines, at major music companies or even as beta testers.)   4$
'$b                                                                         d$'
  '$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$' 
                                                         ||
   _____           ______________________________________||__________________
 z$$$$$$ Radium.is $$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$
J$`                                                                          4$
$F  Seniors : Sandor, Jazzmaster, Whouse                                     4$
$F  Members : Drugstah, Freeform, Finsitez, Visuman, Megadoc, J@ker, Audi0,  4$
$F            Pterra, Smaug, Midiboy, Eetfuk, Lexpure, Taurus, Tuccos,       4$
$F            Coke2, Deepzone, Int69, MadMax, MrJoiz, zound, RickyJ          4$
'$b                                                                         d$'
  '$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$$03/04/98$$$$'
                                                               nfo by sandor


This version of PoINT CDaudio/32 supports the following recording devices
(DAO = disc-at-once).

	- Grundig CDR100IPW
	- HighTech CD-R1002
	- HP 4020
	- HP 6020
	- HP CD-Writer
	- HP 7100		(not DAO, see below !)
	- JVC XR-W1001		(not DAO)
	- JVC XR-W2001		(firmware revision 2.xx for DAO)
	- JVC XR-W2010
	- JVC XR-W2020
	- JVC XR-W2022
	- JVC R2626
	- JVC XR-W2040
	- Kodak PCD200		(not DAO)
	- Kodak PCD225		(firmware revision 1.07 or higher for DAO)
	- Kodak PCD240		(see below)
	- Matsushita CW-7501
	- Matsushita CW-7502	(firmware revision 3.00 or higher)
	- Nomai 680RW
	- Olympus CDS615
	- Olympus CDS620
	- Optima CD-R650
	- Panasonic CW-7501
	- Panasonic CW-7502	(firmware revision 3.00 or higher)
	- Philips CDD521	(not DAO)
	- Philips CDD522	(firmware revision 1.07 or higher for DAO)
	- Philips CDD2000	(see below !)
	- Philips CDD2600
	- Philips CDD3610	(not DAO, see below !)
	- Pinnacle RCD-1000	(firmware revision 2.xx for DAO)
	- Pinnacle RCD5040
	- Pinnacle RCD4X4
	- Pinnacle RCDW226
	- Pioneer DR-R504	(not DAO)
	- Plasmon RF4000	(not DAO)
	- Plasmon RF4100	(not DAO)
	- Plasmon RF4102	(not DAO)
	- Plasmon CDR4220
	- Plasmon CDR4240	(see below !)
	- Plasmon CDR4400
	- Plasmon CDR480	(firmware revision 3.00 or higher)
	- Plextor PX-R412	(firmware level 33 or higher for DAO)
	- Ricoh MP6200S
	- Ricoh MP6201S
	- Ricoh RO-1420		(see below !)
	- SAF CD-R2004
	- SAF CD-R2006		(not DAO)
	- SAF CD-R4006		(see below !)
	- Sony CDU920
	- Sony CDU924
	- Sony CDU926		(not DAO)
	- Sony CDU928		(not DAO, see below !)
	- Teac CD-R50
	- Teac CD-R55		(firmware revision 1.0f or higher for DAO)
	- Yamaha CDR100		(firmware revision 1.04 or higher for DAO)
	- Yamaha CDR102
	- Yamaha CDR200
	- Yamaha CDR400		(see below !)
	- Yamaha CRW4260

