APEG.FEM.2D.v1.0-CF x/1

Here is a powerful module – from the Apeg system intended for solving
planar linear elastic-static tasks using the Finite Element Method. The
user can select the planar stress problem calculation, (the perpendicular
stress component equals zero) and planar deformation, (the perpendicular
deformation component equals zero). The planar stress is suitable for
solving desk solids, where the solid thickness in a perpendicular
direction is relatively small compared to the other solid dimensions. The
planar deformation is designed for solving long prismatic solids stressed
in a certain way, where it is supposed that the perpendicular direction
shift is equal to zero.

Serial: 0000-c2c2
