
This is a image processing demo program using LabVIEW 3.0

By Jicun Zhong 
Dept. of Biomed. Eng. 
Linkoping Univ. 
S-581 85 Linkoping
Sweden

Usage of ImgProc.exe.

1. Run ImgP.exe under DOS. ImgP.exe will self-extract to produce 
   ImgProc.exe, ImgProc.ini, lvdevice.dll, PIMDemo.dat and Readme.txt files.

2. Copy PIMDemo.DAT to your C:\Windows\ directory.

3. Always keep ImgProc.exe, ImgProc.ini and lvdevice.dll at the same place.

4. Run ImgProc.exe under Windows from Program Manager.

Note, your PC should have 8Mb RAM plus some virtual memory and a math coprocessor.
Windows should be running at 256-color mode. Also it will be much better if you 
use SVGA at 1024x768. The PIMDemo.dat is a laser Doppler perfusion image of human 
hand with a small burn on the back. The black thick line in the image is meant for
checking the validity of 2D DFT/FFT on directional analysis. Note, the 2D DFT/FFT
is very memory consuming. Therefore, ImgProc.exe takes 10Mb of memory on start. 
Even so, you may still need to choose 2D DFT/FFT first to see its effects.
