; NEC/AT&T PCMCIA 14.4

;===================================================
; Last revision date: 084/26/94 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 14 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;=====================================================

[attributes]

MODELS=NEC/AT&T PCMCIA 14.4
NULL MODEM=0
MAXIMUM SPEED=57600
DEFAULT SPEED=57600

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0V1
SETUP=ATQ0X6&C1&D2S0=0\\D3
RTS/CTS ENABLED=AT\\Q3&R0
RTS/CTS IGNORED=AT\\Q0&R1
VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX3D
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

NO DIALTONE=NO DIALTONE
NO DIALTONE=NO DIAL TONE

ERROR=ERROR

RING=RING

CONNECT, 57600, 14400=CONNECT 14400
CONNECT, 57600, 14400=CONNECT 14400/EC
CONNECT, 57600, 14400=CONNECT 14400/NoEC
CONNECT, 57600, 14400=CONNECT 14400/V42b
CONNECT, 57600, 14400=CONNECT 14400/V42
CONNECT, 57600, 14400=CONNECT 14400/MNP5
CONNECT, 57600, 14400=CONNECT 14400/MNP4
CONNECT, 57600, 14400=CONNECT 14400/MNP3
CONNECT, 57600, 14400=CONNECT 14400/MNP2

CONNECT, 57600, 12000=CONNECT 12000
CONNECT, 57600, 12000=CONNECT 12000/EC
CONNECT, 57600, 12000=CONNECT 12000/NoEC
CONNECT, 57600, 12000=CONNECT 12000/V42b
CONNECT, 57600, 12000=CONNECT 12000/V42
CONNECT, 57600, 12000=CONNECT 12000/MNP5
CONNECT, 57600, 12000=CONNECT 12000/MNP4
CONNECT, 57600, 12000=CONNECT 12000/MNP3
CONNECT, 57600, 12000=CONNECT 12000/MNP2

CONNECT, 57600, 9600=CONNECT 9600
CONNECT, 57600, 9600=CONNECT 9600/EC
CONNECT, 57600, 9600=CONNECT 9600/NoEC
CONNECT, 57600, 9600=CONNECT 9600/V42b
CONNECT, 57600, 9600=CONNECT 9600/V42
CONNECT, 57600, 9600=CONNECT 9600/MNP5
CONNECT, 57600, 9600=CONNECT 9600/MNP4
CONNECT, 57600, 9600=CONNECT 9600/MNP3
CONNECT, 57600, 9600=CONNECT 9600/MNP2

CONNECT, 57600, 7200=CONNECT 7200
CONNECT, 57600, 7200=CONNECT 7200/EC
CONNECT, 57600, 7200=CONNECT 7200/NoEC
CONNECT, 57600, 7200=CONNECT 7200/V42b
CONNECT, 57600, 7200=CONNECT 7200/V42
CONNECT, 57600, 7200=CONNECT 7200/MNP5
CONNECT, 57600, 7200=CONNECT 7200/MNP4
CONNECT, 57600, 7200=CONNECT 7200/MNP3
CONNECT, 57600, 7200=CONNECT 7200/MNP2

CONNECT, 57600, 4800=CONNECT 4800
CONNECT, 57600, 4800=CONNECT 4800/EC
CONNECT, 57600, 4800=CONNECT 4800/NoEC
CONNECT, 57600, 4800=CONNECT 4800/V42b
CONNECT, 57600, 4800=CONNECT 4800/V42
CONNECT, 57600, 4800=CONNECT 4800/MNP5
CONNECT, 57600, 4800=CONNECT 4800/MNP4
CONNECT, 57600, 4800=CONNECT 4800/MNP3
CONNECT, 57600, 4800=CONNECT 4800/MNP2

CONNECT, 57600,  2400=CONNECT 2400
CONNECT, 57600,  2400=CONNECT 2400/EC
CONNECT, 57600,  2400=CONNECT 2400/NoEC
CONNECT, 57600,  2400=CONNECT 2400/V42b
CONNECT, 57600,  2400=CONNECT 2400/V42
CONNECT, 57600,  2400=CONNECT 2400/MNP5
CONNECT, 57600,  2400=CONNECT 2400/MNP4
CONNECT, 57600,  2400=CONNECT 2400/MNP3
CONNECT, 57600,  2400=CONNECT 2400/MNP2

CONNECT, 57600, 1200=CONNECT 1200
CONNECT, 57600, 1200=CONNECT 1200/EC
CONNECT, 57600, 1200=CONNECT 1200/NoEC
CONNECT, 57600, 1200=CONNECT 1200/MNP5
CONNECT, 57600, 1200=CONNECT 1200/MNP4
CONNECT, 57600, 1200=CONNECT 1200/MNP3
CONNECT, 57600, 1200=CONNECT 1200/MNP2

