;Toshiba T144NW Noteworthy 14.4 Data/Fax Modem

;===============================================
; Last revision date: 11/18/94 (update this date
; each time you edit; it is also advisable to rename
; your edited file [use Save As, rather than Save 
; option] to avoid later confusion and to keep the 
; original .MDM file intact).

; NOTE: Refer to the file TEMPLATE.MDM (A Sample Modem 
; Command File) for a description of modem command 
; files and how they work. "A Sample Modem Command 
; File" is user selectable within the Lotus Notes 
; Setup dialog "Modem Type" listbox in which you found 
; this modem command file (see end of listings, 
; beginning with a period) and is a printable ASCII 
; text file (approximately 14 pages). 

; Additional information may be obtained from either of 
; the two so-called "generic" modem command files 
; (alphabetically listed under letter G, designed for 
; use with Notes Releases 2.x and 3.x, 9600 bps and 
; 14400 bps maximum, respectively), each of which may 
; first be tried as-is with unlisted modems, then edited 
; if required (within the Notes edit box, or outside of 
; Notes, with any text editor) according to the printed 
; instructions within each file, and in compliance with 
; the vendor's command set, result codes, DIP switch 
; settings, and technical specifications as listed in 
; the equipment's users manual.

; For the specific modem(s) listed under this heading:
;=====================================================

[attributes]

MODELS=Toshiba Noteworthy T144NW (beta)
NULL MODEM=0
MAXIMUM SPEED=57600
DEFAULT SPEED=57600

[commands]

ESCAPE=+++
ATTENTION=ATE0V1
HANGUP=ATH0
SETUP=AT&F
SETUP=ATE0V1
SETUP=ATQ0&Q5&C1&D2S0=0S37=0X4
RTS/CTS ENABLED=AT\\Q3
RTS/CTS IGNORED=AT\\Q0
VOLUME OFF=ATM0
VOLUME LOW=ATM1L1
VOLUME MEDIUM=ATM1L2
VOLUME HIGH=ATM1L3
ANSWER=ATA
MANUAL DIAL=ATX3D
AUTO PULSE DIAL=ATDP
AUTO TONE DIAL=ATDT
AUTO DIAL SUFFIX=,

[responses]

OK=OK

BUSY=BUSY

NO ANSWER=NO ANSWER

NO CARRIER=NO CARRIER

NO DIALTONE=NO DIALTONE
NO DIALTONE=NO DIAL TONE

ERROR=ERROR

RING=RING

CONNECT, 57600, 57600=CONNECT 57600
CONNECT, 57600, 57600=CONNECT 57600*
CONNECT, 57600, 57600=CONNECT 57.6*
CONNECT, 57600, 57600=CONNECT 57*

CONNECT, 57600, 38400=CONNECT 38400
CONNECT, 57600, 38400=CONNECT 38400*
CONNECT, 57600, 38400=CONNECT 38.4*
CONNECT, 57600, 38400=CONNECT 38*

CONNECT, 57600, 28800=CONNECT 28800
CONNECT, 57600, 28800=CONNECT 28800*
CONNECT, 57600, 28800=CONNECT 28.8*
CONNECT, 57600, 28800=CONNECT 28*

CONNECT, 57600, 26400=CONNECT 26400
CONNECT, 57600, 26400=CONNECT 26400*
CONNECT, 57600, 26400=CONNECT 26.4*
CONNECT, 57600, 26400=CONNECT 26*

CONNECT, 57600, 24000=CONNECT 24000
CONNECT, 57600, 24000=CONNECT 24000*
CONNECT, 57600, 24000=CONNECT 24.0*
CONNECT, 57600, 24000=CONNECT 24*

CONNECT, 57600, 21600=CONNECT 21600
CONNECT, 57600, 21600=CONNECT 21600*
CONNECT, 57600, 21600=CONNECT 21.6*
CONNECT, 57600, 21600=CONNECT 21*

CONNECT, 57600, 19200=CONNECT 19200
CONNECT, 57600, 19200=CONNECT 19200*
CONNECT, 57600, 19200=CONNECT 19.2*
CONNECT, 57600, 19200=CONNECT 19*

CONNECT, 57600, 16800=CONNECT 16800
CONNECT, 57600, 16800=CONNECT 16800*
CONNECT, 57600, 16800=CONNECT 16.8*
CONNECT, 57600, 16800=CONNECT 16*

CONNECT, 57600, 14400=CONNECT 14400
CONNECT, 57600, 14400=CONNECT 14400*
CONNECT, 57600, 14400=CONNECT 14.4*
CONNECT, 57600, 14400=CONNECT 14*

CONNECT, 57600, 12000=CONNECT 12000
CONNECT, 57600, 12000=CONNECT 12000*
CONNECT, 57600, 12000=CONNECT 12.0*
CONNECT, 57600, 12000=CONNECT 12*

CONNECT,  9600, 9600=CONNECT 9600
CONNECT, 57600, 9600=CONNECT 9600*
CONNECT, 57600, 9600=CONNECT 9.6*
CONNECT, 57600, 9600=CONNECT 96*

CONNECT,  7200, 7200=CONNECT 7200
CONNECT, 57600, 7200=CONNECT 7200*
CONNECT, 57600, 7200=CONNECT 7.2*
CONNECT, 57600, 7200=CONNECT 72*

CONNECT,  4800, 4800=CONNECT 4800
CONNECT, 57600, 4800=CONNECT 4800*
CONNECT, 57600, 4800=CONNECT 4.8*
CONNECT, 57600, 4800=CONNECT 48*

CONNECT,  2400, 2400=CONNECT 2400
CONNECT, 57600, 2400=CONNECT 2400*
CONNECT, 57600, 2400=CONNECT 2.4*
CONNECT, 57600, 2400=CONNECT 24*

CONNECT,  1200, 1200=CONNECT 1200
CONNECT, 57600, 1200=CONNECT 1200*
CONNECT, 57600, 1200=CONNECT 1.2*

CARRIER,,28800=CARRIER 28800

CARRIER,,26400=CARRIER 26400

CARRIER,,24000=CARRIER 24000

CARRIER,,21600=CARRIER 21600

CARRIER,,19200=CARRIER 19200

CARRIER,,16800=CARRIER 16800

CARRIER,,14400=CARRIER 14400

CARRIER,,12000=CARRIER 12000

CARRIER,, 9600=CARRIER 9600

CARRIER,, 7200=CARRIER 7200

CARRIER,, 4800=CARRIER 4800

CARRIER,, 2400=CARRIER 2400

CARRIER,, 1200=CARRIER 1200

