  HOW TO INSTALL THE REMOTE OFFICE CLIENT WITH WINDOWS FOR WORKGROPS 3.11
  -----------------------------------------------------------------------

  WFW requires the NDIS interface into Remote Office.  Fortunately,
  WFW has a very effective setup program which can be instructed to
  modify its configuration files to accomodate Remote Office.

  WINDOWS FOR WORKGROUPS INSTALLED BEFORE REMOTE OFFICE

  If Windows for Workgroups was installed before Remote Office, the
  Remote Office install procedure will copy a file called "OEMROF.INF"
  to the Windows for Workgroups SYSTEM directory.  Once the Remote
  Office install has been run, the following steps must be performed to
  complete the setup:

  1.  Load windows, from Progam Manager,
  2.  Choose the "NETWORK"  icon.
  3.  Choose the "NETWORK SETUP" icon.
  4.  Activate the "Networks" button.
  5.  Select the 2nd radio button, which installs the Windows For
      Workgroups network.
  6.  Select the "No Additional Networks" radio button and press OK.
  7.  From the Network Setup Window, activate the "Sharing" button.
  8.  Select the option to give others access to your files (if desired).
  9.  Select the "Drivers" button.
  10. Remove the current adapter setup.
  11. Choose "ADD ADAPTER".
  12. Select "Stampede Remote Office NDIS Driver".
  13. Remove MicroSoft NETBEUI protocol.
  14. Choose "ADD PROTOCOL".
  15. Select "MicroSoft NETBEUI with Remote Office Parameters".
  16. Remove "IPX/SPX Compatible Transport with NETBIOS".
  17. Continue with the network setup.
  18. See important note below.


  WINDOWS FOR WORKGROUPS NOT INSTALLED BEFORE REMOTE OFFICE

  1.  Install Windows for Workgroups.  (Select no network support).
  2.  Choose the "NETWORK"  icon.
  3.  Choose the "NETWORK SETUP" icon.
  4.  Activate the "Networks" button.
  5.  Select the 2nd radio button, which installs the Windows For
      Workgroups network.
  6.  Select the "No Additional Networks" radio button and press OK.
  7.  From the Network Setup Window, activate the "Sharing" button.
  8.  Select the option to give others access to your files (if desired).
  9.  Select the "Drivers" button.
  10. Remove the current adapter setup.
  11. Choose "ADD ADAPTER".
  12. Select "Unlisted or Updated Network Adapters".
  13. At the prompt for OEMSETUP.INF, enter your Remote Office directory.
  14. Select "Stampede Remote Office NDIS Driver" as the adpater.
  15. Remove MicroSoft NETBEUI protocol.
  16. Choose "ADD PROTOCOL".
  17. Select "MicroSoft NETBEUI with Remote Office Parameters".
  18. Remove "IPX/SPX Compatible Transport with NETBIOS".
  19. Continue with the network setup.

  IMPORTANT:
  Windows for Workgorups may insert a "NET START" line at the
  begining of the AUTOEXEC.BAT file.  If this is the case, remove
  that line.   Use the ROSTART.BAT file located in the ROFFICE
  directory.

  If you wish to load the system using an alternate BAT file, the load
  sequence should be similar to one of the following.

  Ethernet:                            Token-Ring:

  CD\ROF                               CD\ROF
  ROFFICE                              ROFFICE
  NET INIT                             NET INIT
  NDROF-E                              NDROF-T
  RO LOGIN HOST                        RO LOGIN HOST
  NET START NETBEUI                    NET START NETBEUI
  WIN                                  WIN


