Ensoniq Soundscape Install for OS/2

Step #1 :
    You must have the OS/2 Multimedia extensions already loaded on your system
    (indicated by the "Multimedia" icon on your desktop).  If it is installed
    skip to step #2, otherwise continue to step #1A.

    Step #1A :
        Run the "Selective Install" located in the "System Setup" item under
        the "OS/2 System" folder.

    Step #1B:
        After the Install program has been initialized, you will receive the
        "System Configuration" window.  This window will display information
        about how your system is currently configured.  The lower left corner 
        of this window has the "Multimedia Device Support" box that should 
        read "None," - this is correct.  You leave this screen by clicking on 
        the "OK" button.

    Step #1E:
        You should now have the "OS/2 Setup and Installation" window without 
        any of the check boxes selected.  The sixth box from the top is the 
        "Multimedia Software Support" line with the check box at the beginning.
        You should click on this box (it must have the check mark in it), then 
        click the "Install" button to continue.

    Step #1D:
        Follow all of the prompts, and after the install is complete, shut 
        down your system as normal and reboot OS/2, then continue with step #2.
        
Step #2:
    Run the "Multimedia Application Install" program from the "Multimedia" 
    icon window on the desktop.

Step #3:
    Insert the Soundscape OS/2 Install disk (Soundscape Installation Disk, 
    Disk #2) into the drive, then use the drive pull down (the upper left 
    corner) to select the drive letter (A: or B:).

Step #4:
    Click on the "Ensoniq Soundscape" name or the ICON to the left.  This 
    should highlight the line and place a check mark at the beginning of the 
    line.  Then click the "Install" button to continue.

Step #5:
    You should receive a warning saying that the program is going to change 
    your config.sys file.  You should let the program make the modifications 
    for you, otherwise your sound card may not work!  Click the "Yes" button 
    to continue from this point.

Step #6:
    After a brief message indicating that the driver information is being 
    copied you will receive a prompt to "Select the total number of Ensoniq 
    Soundscape."  This prompt is for systems that may have more then one 
    Soundscape installed.  Currently we only support ONE.  Selecting ZERO will 
    uninstall any previous Soundscape installations.

Step #7:
    Set the Soundscape system values as you would in any other system.  The 
    default values should be correct but if you know that these conflict with 
    another device in your system make the change at this point in the install.  
    Use the pull downs to select a different value if necessary.  When all 
    changes (if any were necessary) are completed, click "OK" to continue.

Step #8:
    The installation will now update your system files.  You should receive 
    two more prompts, the first one saying that the config.sys file was backed 
    up and the final one saying that the installation was completed.  Click 
    the "OK" button to clear these prompts.

Step #9:
    After the installation has completed, shut down OS/2 and reboot it so that 
    the changes can take effect.  The Soundscape card should be initialized 
    and you should get the startup sound effects when the desktop appears.
