Chameleon
Technical Tips For Getting Connected

Internet Provider: WLN Internet Services
Service Area: 	Olympia and Seattle, Washington local access
		800 National access

Address:
WLN Internet Services
4224 6th Avenue SE, Bldg. 3
Lacey, WA  98503-1024

Phone: 800-DIAL-WLN
Fax: 206-923-4009
email: info@wln.com (for general information)
       support@wln.com (for technical support)

General Notes:
WLN uses dynamic IP addressing. Users should enter a dummy
IP address of 1.1.1.1

Chameleon Pre-configured access type: SLIP

The phone number for SLIP access: 
The phone number for support: 

Domain Name Server(s) are: 
192.156.252.2

POP3 Server:

NNTP News Server:

The script for a SLIP connection should be as follows. 
(The [name] entry will correspond to the name of the 
interface the user defined in custom, if not using a 
pre-configured setup.  The  slip.ini file is found in 
the netmanag directory.)

[WLN]
SCRIPT=-n $r Login: $u$r word: $p$r ==> $c$r -i
TYPE=SLIP

Following is the LOG from Custom for a successful connection:

ATQ0V1E0M1
OK
ATS0=0
OK
ATDT9,1-206-923-4082
CONNECT 9600/ARQ/V32/LAPM

AL WLN

      Lacey, WA  98503-0888              FAX:  206-923-4009

         E-Mail:  info@wln.com       (for general information)
                  support@wln.com    (for technical support)

Annex CLI  Copyright 1991 Xylogics, Inc.
IBM AIX Version 3 for RISC System/6000  Copyright by IBM and others 1982, 1991
Pine  Copyright 1989, 1990, 1991, 1992 University of Washington
Login: (deleted)
Password:******

Permission granted

      WLN Terminal Server Options

      1.  WLN Easy Access
      2.  WLN Internet Services Menu
      3.  Telnet protocol
      4.  SLIP mode
      5.  Terminate session and hangup

      Please enter your selection (1-5) below:

      ==>SLIP
SLIP
192.156.252.122
