Chameleon
Technical Tips For Getting Connected

Last Updated: 7/12/94

Internet Provider: PSI
Service Area: Nationwide local access phone numbers

Address:
Performance Systems International
510 Huntmar Park Drive
Herndon, VA 22070

Phone: 703-904-4100
Fax: 703-904-4200

General Notes:
Chameleon Pre-configured access type: SLIP

Please note that the "Chameleon Sampler" will not work with 
PSI's new InterRamp service that features ISDN and 14.4
dialup access.  Only the latest version of Internet Chameleon
will work with the new InterRamp service.

Uses Dynamic IP substitution. Pre-configured custom .cfg 
has a dummy IP address of 1.1.1.1

The phone number for SLIP access is: various local numbers
The phone number for support is: 518-283-8860

Domain Name Server(s) are: 
38.145.250.2
38.146.21.2
192.33.4.10


The script for a SLIP connection should be as follows. 
(The [name] entry will correspond to the name of the 
interface the user defined in custom, if not using a 
pre-configured setup.  The  slip.ini file is found in 
the netmanag directory.)

[PSINet]
SCRIPT=name: $u$r word: $p$r -n $6$c$r -i
TYPE=SLIP

Following is the LOG from Custom for a successful connection:

ATQ0V1E0
OK
ATS0=0
OK
ATDT9,986-1266
CONNECT 9600/ARQ/V32/LAPM

Username:(deleted)
Password:*******
SLIP

psinet_ts>SLIP
Entering SLIP mode.
Your IP address is 38.145.222.233. 