Chameleon
Technical Tips For Getting Connected
 
Internet Provider: HookUp Communication Corporation 

Service Area: Toronto and surrounding, Waterloo, Ottawa (CANADA)
 
Address: 
HookUp Communication Corporation
1075 North Service Road West
Oakville, ON 
L6M 2G2

Phone: 905-847-8000
Fax: 905-847-8420
email: info@hookup.net, support@hookup.net

General Notes:
 
Chameleon Pre-configured access type: PPP
(Note the choice of PPP is hardwired into the slip script below.)

The phone number(S) for SLIP access: 
Toronto: 416-630-0970
Oakville: 905-847-8866
Burlington: 905-333-3568
Mississauga: 905-276-6179
Hamilton: 905-526-8755
Kitchener-Waterloo: 519-883-4665
Hespeler: 519-658-6448
Galt: 519-621-7855
Lynden: 519-647-3570
Ottawa: 613-526-5636

The phone number for support: 905-847-8577
 
Domain Name Server(s) are: 
Toronto: noc.tor.hookup.net (165.154.1.1)
Ottawa: nic.ott.hookup.net (165.154.5.1)
Waterloo: nic.hookup.net (198.133.162.1)

Secondary: medusa.hookup.net (198.133.162.8)
Secondary: relay.tor.hookup.net (165.154.1.8)
 
POP3 Server:
Toronto: noc.tor.hookup.net (165.154.1.1)
Ottawa: nic.ott.hookup.net (165.154.5.1)
Waterloo: nic.hookup.net (198.133.162.1)
 
NNTP News Server:
Toronto: nnrp.tor.hookup.net 
Ottawa: nnrp.ott.hookup.net
Waterloo: nnrp.hookup.net
 
The script for a SLIP connection should be as follows. 
(The [name] entry will correspond to the name of the 
interface the user defined in custom, if not using a 
pre-configured setup.  The  slip.ini file is found in 
the netmanag directory.)

SCRIPT=login: $u$r word: $p$r choice: $c$r
TYPE=PPP
 
Following is the LOG from Custom for a successful connection:

ATQ0V1E0M1ATQ0V1E0M1OK
ATS0=0
OK
ATDT9,1-905-847-8866
CONNECT 9600/ARQ/V32/LAPM

noc
Welcome to HookUp Communications.noc!login:(deleted)
Password:********


1. Shell (command line)
2. Slip
3. PPP

Enter 1-3 for choice:3
