Chameleon
Technical Tips For Getting Connected

Last Updated: 6/28/94

Internet Provider: Prometheus Information Network Group, Inc.	
Service Area: U.S., U.S. Virgin Islands, Puerto Rico

Address: 400 Perimeter Center Terrace
	 Suite 155 North
	 Atlanta, GA  30346

Phone: (404) 399-1670 / (800) PING TEL
Fax: (404) 399-1671
email: questions@ping.com
 
General Notes:
 
Chameleon Pre-configured access type: PPP
 
The phone number for SLIP access: (800) PING 003  /  (404) 481-6700
The phone number for support: (800) PING TEL
Email address for support: support@ping.com
 
Domain Name Server(s) are: 
ns.ping.com 		(166.78.1.2)
mathcs.emory.edu 	(128.140.110.1)
noc.sura.net 		(192.80.214.100)
 
POP3 Server: ping.ping.com
 
NNTP News Server: news.ping.com

The script for a SLIP connection should be as follows. 
(The [name] entry will correspond to the name of the 
interface the user defined in custom, if not using a 
pre-configured setup.  The  slip.ini file is found in 
the netmanag directory.)

[Ping Internet]
SCRIPT=login: $u$r word: $p$r enabled $2$r
TYPE=PPP
 
Following is the LOG from Custom for a successful connection:

ATQ0V1E0M1
OK
ATS0=0
OK
ATDT9,1-800-746-4003
CONNECT 14400/ARQ/V32/LAPM/V42BIS


Telebit's NetBlazer Version 2.3

terrace1 login:(deleted)
Password:********


Packet mode enabled
