


             IMPORTANT PRINTER DRIVER INSTALLATION INSTRUCTIONS

                      LOTUS(R) 1-2-3(R) RELEASE 2.3/2.4
                         HP LASERJET 5P PRINTER


     INSTALLING AND SELECTING A PRINTER DRIVER

     Use the following steps to install and select your HP LaserJet 5P
     printer driver for Lotus 1-2-3 release 2.3/2.4:

     1.   Copy the printer driver files using the SETUP program.

     2.   At a DOS prompt on the drive where Lotus 1-2-3 is loaded, type
          CD\ followed by the name of the subdirectory where Lotus 1-2-3 
          is loaded (for example, CD\123r23) to change to the Lotus 1-2-3 
          subdirectory, then press [Enter].

          At the DOS prompt, type LOTUS and press [Enter] to bring up
          the "Lotus 1-2-3 Access Menu."

          Use your cursor keys to highlight INSTALL on the "Lotus 1-2-3
          Access Menu," then press [Enter] to run the INSTALL program.

     3.   Read the instructions on the LOTUS INSTALL PROGRAM screen,
          then press [Enter].

     4.   Select CHANGE SELECTED EQUIPMENT on the MAIN MENU, then press
          [Enter].

     5.   Select ADD NEW DRIVERS TO THE LIBRARY on the CHANGE SELECTED
          EQUIPMENT menu, then press [Enter].

     6.   Specify the drive containing the update disk (A or B), then
          press [Enter].

     7.   Select MODIFY THE CURRENT DRIVER SET on the CHANGE SELECTED
          EQUIPMENT menu, then press [Enter].

     8.   Select GRAPHICS PRINTER on the MODIFY CURRENT DRIVER SET menu,
          then press [Enter].

     9.   Select HP on the GRAPHICS PRINTER SELECTION menu, then press
          [Enter].

     10.  Select LASERJET 4 SERIES PCL 5" then press [Enter].  (The drivers
          are not necessarily listed in alphabetical order.)  You will
          return to the MODIFY CURRENT DRIVER SET menu.

     11.  Select RETURN TO PREVIOUS MENU on the MODIFY CURRENT DRIVER
          SET menu, then press [Enter].

     12.  Select SAVE THE CURRENT DRIVER SET on the CHANGE SELECTED
          EQUIPMENT menu, then press [Enter].

                                      Lotus 1-2-3 Release 2.3/2.4      1



     13.  Read the instructions on the SAVING YOUR CHANGES screen, then
          press [Enter].

     14.  Read the instructions on the GENERATING FONTS screen, then
          press [Enter].

     15.  Select the set of font sizes you want to use with WYSIWYG on
          the GENERATING FONTS menu.  Choose "Basic," "Medium," or
          "Extended" depending on the font sizes you need and the amount
          of disk space you have available.  The box on the GENERATING
          FONTS menu gives information about disk space requirements.
     _______________

     NOTE   "Basic" gives a maximum font point size of 24, "Medium" a
            maximum font point size of 36, and "Extended" a maximum font
            point size of 72.  The larger the set of fonts, the more
            disk space will be required.
     _______________

     16.  After you select the font set, press [Enter], and a GENERATING
          FONTS screen will display while fonts are being made.  When
          font generation is complete, press any key to end Install.
     _______________

     NOTE   You have just installed a WYSIWYG printer driver.  To use
            this driver, you need to enable WYSIWYG within Lotus 1-2-3.
            (See the next section "Enabling WYSIWYG" for instructions.)

            Install the HP LaserJet series text printer driver if you
            plan to use setup strings or print multiple ranges on a
            page; and install the LaserJet III, IIID, and IIIP graphics
            printer driver if you plan to use the Lotus 1-2-3 PrintGraph
            feature.  See your Lotus 1-2-3 release 2.3/2.4 user's
            documentation for information about how to install these
            drivers.
     _______________

     ENABLING WYSIWYG

     To use WYSIWYG, you must load it into memory.  WYSIWYG can be added
     automatically upon entering Lotus 1-2-3 or invoked during the
     current Lotus 1-2-3 session.  The following instructions apply to
     adding WYSIWYG during a Lotus 1-2-3 session.  Check the Lotus 1-2-3
     documentation for instructions about loading WYSIWYG automatically.

     1.   Start Lotus 1-2-3.

     2.   To enable WYSIWYG, hold down the [Alt] key on your computer's
          keyboard, then press the [F10] key.

     3.   Select [A]ttach.

     4.   Highlight WYSIWYG.ADN, then press [Enter].



                                      Lotus 1-2-3 Release 2.3/2.4      2



     5.   Select "No Key" if you plan to use [:] (colon) or use a mouse
          to display the WYSIWYG main menu.  This WYSIWYG function may
          also be assigned to [Alt-F7], [Alt-F8], [Alt-F9] or [Alt-F10].
          After making your selection, the WYSIWYG add-in program will
          load into memory.  Press [Q]uit to return to the Lotus 1-2-3
          spreadsheet screen.
     _______________

     NOTE   Press [:] (colon) or press the alternate key you chose
            during the add-in process to activate the WYSIWYG menu.  To
            use Lotus 1-2-3 menus and functions, use the [/] key.
     _______________

     SELECTING A PRINTER

     To choose a printer, press [:] [P]rint [C]onfig [P]rinter.  Select
     the HP LaserJet printer you installed, press [Enter], then
     press [Q]uit twice to return to your spreadsheet.

     LOTUS 1-2-3 FOR DOS RELEASE 2.3/2.4 NETWORK EDITION

     If you are a network administrator and need to update the printer
     driver for the Lotus 1-2-3 for DOS Release 2.3/2.4 Network Edition,
     you will need the Lotus 2.3/2.4 Network Edition update disk.  This
     disk is available electronically from the HP Peripherals Forum on
     CompuServe, from Hewlett-Packard Distribution at (303) 353-7650, or
     from Lotus Development Corporation.


     LOTUS DEVELOPMENT CORPORATION CUSTOMER SUPPORT

          Customer Support Number..................(900) 454-9009
          Hours.............................9 AM to 6 PM, M-F EST
          Charge.........First minute free, $2 subsequent minutes
          "Prompt" Member Support..................(800) 223-1662
          Hours...........................24 hours, 7 days a week
          Required Identification................Member ID number




        Lotus(r) 1-2-3(r) is a registered trademark
             of Lotus Development Corporation.

           Copyright(c) Hewlett-Packard Co. 1995
  This information is subject to change without notice and
           is provided "as is" with no warranty.
    Hewlett-Packard shall not be liable for any direct,
   indirect, special, incidental or consequential damages
        in connection with the use of this material.






                                      Lotus 1-2-3 Release 2.3/2.4      3
