Amberlogic Mistral                              S0=0 Q0V1 F7 N0 &E0 &K5                         AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
AncH0r Signalman Lightning 24                   S0=0 Q0 V1 X4 F1                                AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
AncH0r 2400E                                    S0=0 Q0 V1 X4 F1                                AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
AncH0r 96E4                                     S0=0 Q0 V1 X4\N3\V1%C0\Q3&C1&D2                 AT  Z   H0  OK  CONNECT  NO CARRIER 9600  |
ATI 9600 ETC                                    S0=0 Q0 V1X4&Q0&U0&K4&C1&D2                     AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
AT&T 4024                                       S0=0 Q0 V1 X1                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Best Data - Smart One 96/24                     S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Best Data - Smart One 1442F                     S0=0 Q0 V1 &C1&D2 S11=55\N0&K4&Q5               AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Best Data - Smart One 1442FX                    S0=0 Q0 V1 &C1&D2\N0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Best Data - Smart One V.fast External           S0=0 Q0 V1 &C1&D2\N0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Best Data - Smart One V.fast Internal           S0=0 Q0 V1 &C1&D2 S11=55\N0&K4&Q5               AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Best Data - Smart One ACE 5000                  S0=0 Q0 V1 &C1&D2 \N0\N7%C1"H3                  AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Boca Fax Modem FM9624                           S0=0 Q0 V1 &C1&D2\N0\Q1\N3%C1                   AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
BT V.32                                         S0=0 Q0 V1 &C1&D2E1&EO&K0&M                     AT  Z   H0  OK  CONNECT  NO CARRIER 9600  |
Cardinal MVP24I/MVP24IF                         S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Cardinal 9600/V32                               S0=0 Q0 V1 &C1&D2 &M0                           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
CMS                                             \N1 S0=0 Q0 V1                                  AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Compudyne 9642/V32                              S0=0 Q0 V1 &Q0 &C1&D2                           AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
CTS 2424ADH PLUS                                S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
CTS 2424CTSSM06                                 S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Dataflex Comfax II                              S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Dataflex Dynalink                               S0=0 Q0 V1 B0                                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Dataflex Quadcom                                S0=0 Q0 V1 &C1&D2 %C0 S37=59&C1&D2              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Digicom 9624 Series                             S0=0 Q0 V1 &C1&D2*S1*E0*F2*E5                   AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Digicom Connection Series                       S0=0 Q0 V1 \N0&K4\N5                            AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Digicom Eagle                                   S0=0 Q0 V1 &C1&D2*S1*E0*F2*E9                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Digicom Scout Series                            S0=0 Q0 V1 &C1&D2*E0*F2*E9                      AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
DoveFax 144E 14.4/9.6                           S0=0 Q0 V1 &D2*E0&Q5                            AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dowty Jaguar Quartet L                          S0=0 Q0 V1 E1                                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Dowty Mayze                                     S0=0 Q0 V1 &E0 &C1&D2 X6                        AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dowty Quantum 96                                S0=0 Q0 V1 &E0 %C0 S7=60                        AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dowty Quattro SB2422                            S0=0 Q0 V1E1X1 &E0                              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Dowty Quattro 96                                S0=0 Q0 V1 E1%K0                                AT  &F1 H0  OK  CONNECT  NO CARRIER 9600  |
Dr. Neuhaus FURY 9601 TI                        B15&C1&D2\N3\Q3\J0\N3%C1                        AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Dr. Neuhaus FURY 14.4 TI                        B15&C1&D2\N6\Q3\J0\C1\N6%C1                     AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dr. Neuhaus FURY CARD 14.4                      B15&C1&D2\N6\Q3\J0\C1\N6%C1                     AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dr. Neuhaus FURY 19.2 TI                        B15&C1&D2\N6\Q3\J0\C1\N6%C1                     AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dr. Neuhaus SMARTY 24 PC                        &Q5S46=136%C1                                   AT  &F3 H0  OK  CONNECT  NO CARRIER 2400  |
Dr. Neuhaus SMARTY 24 TI                        &Q5S46=136%C1                                   AT  &F3 H0  OK  CONNECT  NO CARRIER 2400  |
Dr. Neuhaus SMARTY 14.4 TI                      B15&C1&D2\N6\Q3\J0\N6%C1                        AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Dr. Neuhaus SMARTY 19.2 TI                      B15&C1&D2\N6\Q3\J0\N6%C1                        AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
ELSA MicroLink 14.4                             S0=0 %C0 \N0\N3%C3                              AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
ELSA MicroLink 2460                             S0=0 %C0 \N0\N3%C3                              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
ELSA MicroLink 2440                             S0=0 %C0 \N0\N3%C3                              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
ELSA MicroLink 24ooo/288oo                      S0=0 %C0 \N0\N3%C3                              AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Everex Evercom 24E MNP                          S0=0 Q0 V1 &C1&D2\N0\Q1\N3%C1                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Everex Evercom II-24 PS/2                       S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Everex EverFax 2496E                            S0=0 Q0 V1 &C1&D2%C0~                           AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Falcom FCM2400                                  S0=0 Q0 V1 X6&C1&D2                             AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Gateway 2000 Telepath II                        S0=0 Q0 V1 &M0&A3&B1&H2&R1X4S11=55&M4           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Gateway 2000 24/96 PCMCIA                       S0=0 Q0 V1 &Q6&C1&D2S7=60S11=55S95=3&K4&Q5      AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Gateway 2000 Nomad 9600SR                       S0=0 Q0 V1 &C1&D2\N0W2S7=60S11=55\Q1N7          AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
GVC Powerport Bronze                            S0=0 Q0 V1 &C1&D2X1                             AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
GVC Powerport Gold/Silver                       S0=0 Q0 V1 &C1&D2\V1\Q3\J0\N0X1 \N7             AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
GVC Teleport Bronze                             S0=0 Q0 V1 &C1&D2X1                             AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
GVC Teleport Gold/Silver                        S0=0 Q0 V1 &C1&D2\N0\N3                         AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Hayes Compatible (default)                      S0=0 Q0 V1 &C1&D2&K4&Q5                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Hayes V-Series (all)                            S0=0 Q0 V1 &C1&D2&Q5&K4                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Hayes Optima 24/Ultra 24                        S0=0 Q0 V1 &C1&D2&Q5&K4                         AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Hayes Optima 96/Ultra 96                        S0=0 Q0 V1 &C1&D2&Q5&K4                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Hayes Optima 144/Ultra 144                      S0=0 Q0 V1 &C1&D2&Q5&K4                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Info Runner VP9624                              S0=0 Q0 V1 %C0&C1&D2                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Intel SatisFAXtion Modem/100                    S0=0 Q0 V1 &C1                                  AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Intel SatisFAXtion Modem/200                    S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Intel SatisFAXtion Modem/400                    S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Intel SatisFAXtion Modem/400c                   S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Intel 14.4EX Modem                              S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Intel 144e Faxmodem                             S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Intel 144i Faxmodem                             S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Intel PCMCIA Faxmodem 2400/9600                 S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Intel PCMCIA Faxmodem 9600/9600                 S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Intel PCMCIA Faxmodem 14.4/14.4                 S0=0 Q0 V1 \N0\Q1\N3                            AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
LightCom 14.4F                                  S0=0 Q0 V1 &C1&D2%C0                            AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Lightspeed 2400LE                               S0=0 Q0 V1 &C1&D2X4\N3\J0\Q3\V1%C0              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Master Systems Turbo                            S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Megahertz C596FM/Z396FM/IC196FM                 S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N7           AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Megahertz P2144(AA bat.)                        S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N7           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Megahertz P2144(9V)                             S0=0 Q0 V1 &C1&D2&Q0&K4&S1W2S95=18&Q5           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Megahertz P224FMV(AA)/T324FM/C524FM             S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N3           AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Megahertz P296FMV(AA bat.)/T396FM               S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N7           AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Megahertz P224FMV(9V)                           S0=0 Q0 V1 &C1&D2&Q0&K4&S1W2S95=18&Q5           AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Megahertz P296FMV(9V)                           S0=0 Q0 V1 &C1&D2&Q0&K4&S1W2S95=18&Q5           AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Megahertz PCMCIA CC324FM/XJ124FM                S0=0 Q0 V1 &C1&D2&Q0&K4&S1W2S95=18&Q5           AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Megahertz PCMCIA CC3144/XJ1144                  S0=0 Q0 V1 &C1&D2&Q0&K4&S1W2S95=18&Q5           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Megahertz T3144/C5144/Z3144                     S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N7           AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Megahertz Z324FM/IC124FM/TX324FM                S0=0 Q0 V1 &C1&D2\V1\G0\N0\Q1\J0W2\N3           AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Microcom QX4232hs                               S0=0 Q0 V1 &C1&D2&M0%C0                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Miracom Courier HST                             S0=0 Q0 V1 &C1&D2S7=58 X6&B1&H1&R2              AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Motorola UDS                                    S0=0 Q0 V1 &C1&D2\N0\C0\J0\Q1                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Multi-Tech MT224 Series                         S0=0 Q0 V1 &C1&D2 X4&E0&E5$BA0E1S7=60&E1&E15    AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Multi-Tech MT932 Series                         S0=0 Q0 V1 &C1&D2 X4&E0&E5$BA0E1S7=60&E1&E15    AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Multi-Tech MT1432 Series                        S0=0 Q0 V1 &C1&D2 X4&E0&E5$BA0E1S7=60&E1&E15    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Multi-Tech MT1932 Series                        S0=0 Q0 V1 &C1&D2 X4&E0&E5$BA0E1S7=60&E1&E15    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Multi-Tech MultiModem Series II                 S0=0 Q0 V1 &C1&D2 X4&E0&E5$BA0E1S7=60&E1&E15    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
National Semiconductor TyIN 2000                S0=0 Q0 V1E1 &C1&D2\N0&K1;+FCLASS=0\N6          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
National Semiconductor TyIN 4000                S0=0 Q0 V1E1 &C1&D2\N0&K1;+FCLASS=0\N6          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
NEC Laptop                                      S0=0 Q0 V1 &C1&D2\K0\Q1%C0                      AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
OKitel 9600                                     S0=0 Q0 V1 &C1&D2\V1\N3X4&B0&K0S27=128          AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Pace                                            S0=0 Q0 V1 E1 S53=2                             AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Pace Eurolink                                   S0=0 Q0 V1 E1 S53=2                             AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Pace Linnet FX                                  S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Pace Linnet V.32 Quad                           S0=0 Q0 V1 &C1&D2&K4 \P1 F6                     AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Pace Microlin                                   S0=0 Q0 V1 &C1&D2\N0\Q1\N3%C1                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Pace V.32                                       S0=0 Q0 V1 &C1&D2 &K2 \P0                       AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Practical Periph. PM 9600FXMT                   S0=0 Q0 V1 &Q0&K4&Q5                            AT  &F1 H0  OK  CONNECT  NO CARRIER 19200 |
Practical Periph. PM 9600SA                     S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Practical Periph. PC288LCD                      S0=0 Q0 V1 &Q0&K4&Q5                            AT  &F1 H0  OK  CONNECT  NO CARRIER 19200 |
Practical Periph. PC288SA                       S0=0 Q0 V1 &Q0&K4&Q5                            AT  &F1 H0  OK  CONNECT  NO CARRIER 19200 |
Practical Periph. PM 14400FXMT                  S0=0 Q0 V1 &Q0&K4&Q5                            AT  &F1 H0  OK  CONNECT  NO CARRIER 19200 |
Practical Periph. PM 14400FXSA                  S0=0 Q0 V1 &Q0&K4&Q5                            AT  &F1 H0  OK  CONNECT  NO CARRIER 57600 |
Prometheus Promodem 9.6                         S0=0 Q0 V1 &C1&D2*F2                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Prometheus Ultima 9600                          S0=0 Q0 V1 &C1&D2\N0\Q0\J0                      AT  &F  H   OK  CONNECT  NO CARRIER 9600  |
Psion Dacom Quad                                B0 F3 &K1 &C1&D2V1E1Q0                          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Quickcom V.32                                   S0=0 Q0 V1 *E0*F1                               AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Quicktel Zeba 9600 HV/XV                        S0=0 Q0 V1 &C1&D2E1L1X4S7=60\N1\N3              AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Quicktel Zeba 9600 LH/LX                        S0=0 Q0 V1 &C1&D2E1L1X4S7=60                    AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Quicktel Zeba 9624 HV/XV                        S0=0 Q0 V1 &C1&D2E1L1X4S7=60\N1\N3              AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Quicktel Zeba 9696 HV/XV                        S0=0 Q0 V1 &C1&D2E1L1X4S7=60\N1\N3              AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Quicktel Zeba 1414 HV/XV                        S0=0 Q0 V1 &C1&D2E1L1X4S7=60\N1\N3              AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Quicktel Zeba 9624LP, Pocket                    S0=0 Q0 V1 &C1&D2E1L1X4S7=60                    AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Racal Maxam V+                                  S0=0 Q0 V1 &E0 \C4 &C1&D2X1                     AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Reveal PM 100 Int                               S0=0 Q0 V1 &C1&D2 L3E1                          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Reveal PM 200 Int                               S0=0 Q0 V1 &C1&D2 L3E1                          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Reveal PM 250 Ext                               S0=0 Q0 V1 &C1&D2 L2E1                          AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Reveal PM 500 Int                               S0=0 Q0 V1 &C1&D2 L2E1\N0\G1\N3                 AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Reveal PM 550 Ext                               S0=0 Q0 V1 &C1&D2 L2E1\N0\G1\N3                 AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Shiva                                           S0=0 Q0 V1 &M0&C1&D2                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
SupraCOMcard 144                                S0=0 Q0 V1 \N0&K4\N3                            AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
SupraFAXModem Plus                              S0=0 Q0 V1 \N0&K4\N3                            AT  &F2 H0  OK  CONNECT  NO CARRIER 2400  |
SupraFAXModem V.32(bis)/144LC                   S0=0 Q0 V1 \N0&K4\N3                            AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
SupraFAXModem 144i                              S0=0 Q0 V1 \N0&K4\N3                            AT  &F2 H0  OK  CONNECT  NO CARRIER 57600 |
SupraFAXModem 288/288i/288PB                    S0=0 Q0 V1 \N0&K4\N3                            AT  &F2 H0  OK  CONNECT  NO CARRIER 57600 |
Swan 24/96 Fax Modem                            S0=0 Q0 V1 \N0                                  AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Tandata TM500                                   S0=0 Q0 V1 &C1&D2E1X1                           AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Tandy 25-3532                                   S0=0 Q0 V1 &C1&D2-K0 &K4 \N0 %C0                AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Telebit T1600                                   S0=0 Q0 V1 &C1&D2S180=0                         AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Telebit T2500                                   S0=0 Q0 V1 &C1&D2S58=3 S95=0X4                  AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Telebit Other                                   S0=0 Q0 V1 &C1&D2S180=0                         AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Toshiba 1600                                    S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Tricom Business Administrator                   S0=0 Q0V1 &C1&D2X1                              AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Tricom Tempest Quin                             S0=0 Q0V1&C1&D2E1                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Tricom Tornado 5/42                             S0=0 Q0 V1 &C1&D2\N2\J0\V1\Q3                   AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Tricom Tornado 12/42                            S0=0 Q0 V1 &C1&D2%C0\N4                         AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Twincom 24/96 Fax                               S0=0 Q0 V1 &C1&D2&Q0                            AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Twincom 96/42i                                  S0=0 Q0 V1 &C1&D2\N0&K4                         AT  Z   H0  OK  CONNECT  NO CARRIER 9600  |
U.S. Robotics Courier V.32/V.32bis              S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
U.S. Robotics Courier HST                       S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
U.S. Robotics Dual Standard                     S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
U.S. Robotics Dual Standard (UK only)           S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
U.S. Robotics Sportster 9600                    S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
U.S. Robotics Sportster Fax 14,400              S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 57600 |
U.S. Robotics/Touchbase 2496                    S0=0 Q0 V1 &C1&D2\N1\Q1\J1\N3%C1                AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
U.S. Robotics Worldport 14,400                  S0=0 Q0 V1 &C1&D2B0&B1&M4&H2&I2                 AT  &F2 H0  OK  CONNECT  NO CARRIER 19200 |
UST 9600                                        S0=0 Q0 V1 &C1&D2B0&A3&B1&K3&N0                 AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Viva 2442e/2496ef                               S0=0 Q0 V1 &C1&D2N0\N0&K4&Q5                    AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Viva 2442if                                     S0=0 Q0 V1 &C1&D2\N0\Q1\N7                      AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Viva 9642e/9642i                                S0=0 Q0 V1 &C1&D2N0\N0&K4&Q5                    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Viva 14.4K/FAX                                  S0=0 Q0 V1 &C1&D2N0\N0&K4&Q5                    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Viva 14.4i/FAX                                  S0=0 Q0 V1 &C1&D2N0\N0&K4&Q5                    AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Wang                                            S0=0 Q0 V1 &C1&D2&M0                            AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Worldport 24/96                                 S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
WS3000 II                                       S0=0 Q0 V1 &C5&D2X5 &I1 %C0                     AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Zenith Quad                                     S0=0 Q0 V1 B0&C1&D2X2                           AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
ZIFF 144                                        S0=0 %C0 \N0\N3%C3                              AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Zoltrix 14/14                                   S0=0 Q0 V1 &C1&D2W2&Q0&Q5                       AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Zoltrix 96/24                                   S0=0 Q0 V1 &C1&D2W2&Q0&Q5                       AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Zoom 2400                                       S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Zoom 2400 w/V.42bis                             S0=0 Q0 V1 &C1&D2&Q0&K4\&Q5                     AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Zoom 2400 PKT                                   S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 2400  |
Zoom 96/24 Fax Modem                            S0=0 Q0 V1 X4                                   AT  Z   H0  OK  CONNECT  NO CARRIER 9600  |
Zoom 96/24 V.42bis Fax Modem                    S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Zoom V.32                                       S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 9600  |
Zoom V.32bis (14.4)                             S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 57600 |
Zoom PKT 14.4 Pocket                            S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
Zoom PBK 14.4                                   S0=0 Q0 V1 &C1&D2&Q0&K4&Q5                      AT  &F  H0  OK  CONNECT  NO CARRIER 19200 |
ZyXEL U-Series Modems                           S0=0 Q0 V1 &C1&D2&K0&H4&K4                      AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
Other                                           S0=0 Q0 V1 &C1&D2                               AT  &F  H0  OK  CONNECT  NO CARRIER 2400  |
