> # UMAX PowerLook scanners

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

UMAX scanners
Power Look series:
Name | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Optical resolution
PowerLook | PS-2400X | ? | X |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
PowerLook II | PL-II | ? | UTA-II |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Power Look III | PowerLook III | all (1.7) | UTA-III |  | ok | ok | ok | 1,8,12,14,24,36,42 | 1200 x 2400
PowerLook 270 | Color Filmscanner____1 | ? | incl |  | bad | bad | bad | 1,8,14,24,42 | 2700 x 2700
PowerLook 270plus | unknown | ? | incl |  | bad | bad | bad | 1,8,14,24,42 | 2700 x 2700
PowerLook 1100 | unknown | ? * | incl |  | ? | ? | ? | 1,8,14,24,42 | 1200 x 2400
PowerLook 2000 | PowerLook 2000 | ? | UTA-2000 |  | ? | ? | ? | 1,8,12,24,36 | 1000 x 2000
PowerLook 2100XL | unknown | ? | UTA-2100XL |  | ? | ? | ? | 1,8,14,24,42 | 800 x 1600
PowerLook 3000 | PowerLook 3000 | all (2.0) | incl |  | ok | ok | ok | 1,8,14,24,42 | 1220 x 3048 3048 x 3048

* Powerlook 1100 is a firewire scanner: not tested
UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner, incl = is included)

This page has been changed on 16th. decemnber 2001

> Author: Oliver Rauch