sane-xerox_mfp(5)

NAME
sane-xerox_mfp - SANE backend for Xerox Phaser 3200MFP device

DESCRIPTION
The sane-xerox_mfp library implements a SANE (Scanner Access Now Easy) backend that provides access to the following USB and network multifunction-peripheral:

    Phaser 3200MFP
    Dell MFP Laser Printer 1815dn
    Xerox Phaser 6110MFP
    Samsung CLX-3170fn & CLX-3175FW
    Samsung SCX-4200
    Samsung SCX-4300
    Samsung SCX-4500
    Samsung SCX-4500W
    Samsung SCX4725-FN
    Xerox WorkCentre 3119 Series

If you own a scanner other than the ones listed above that works with this backend, please let us know this by sending the scanner's exact model name and the USB vendor and device ids (e.g. from /proc/bus/usb/devices, sane-find-scanner or syslog) to us. Even if the scanner's name is only slightly different from the models mentioned above, please let us know.

CONFIGURATION
/sane/etc/sane.d/xerox_mfp.conf USB scanners do not need any configuration. For SCX-4500W in network mode you need to specify

    tcp host_address [port]

The host_address is passed through resolver, thus can be a dotted quad or a name from /etc/hosts or resolvable through DNS.

FILES

/sane/etc/sane.d/xerox_mfp.conf
    The backend configuration file. By default all scanner types/models are enabled, you may want to comment out unwanted.

/sane/lib/sane/libsane-xerox_mfp.a
    The static library implementing this backend.

/sane/lib/sane/libsane-xerox_mfp.so
    The shared library implementing this backend (present on systems that support dynamic loading).

ENVIRONMENT
SANE_DEBUG_XEROX_MFP If the library was compiled with debug support enabled, this environment variable controls the debug level for this backend. Higher debug levels increase the verbosity of the output. Example: export SANE_DEBUG_XEROX_MFP=4

AUTHOR
Alex Belkin <abc@telekom.ru> Samsung SCX-4500W scan over network support Alexander Kuznetsov <acca(at)cpan.org>

BUGS:
Multicast autoconfiguration for LAN scanners is not implemented yet. IPv6 addressing never been tested.

SEE ALSO
sane(7), sane-usb(5)