> # Not listed UMAX scanners

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

> The sane-umax library implements a SANE backend that provides access to several UMAX-SCSI-scanners. Parallel- and USB- scanners are not supported!

> If you own a UMAX-SCSI-scanner that is not listed as supported, it may work with SANE. It depends on the information the scanner returns to the umax-backend. If the data-block is large enough, the backend prints a warning and continues, but it is possible that not everything works fine.

> I suggest you hold one hand on the power-button of the scanner while you try the first scans!

This page has been changed on 12th. february 2001

> Author: Oliver Rauch