> # UMAX Astra scanners

- Index
- Frontend options:
  - Standard options
  - Advanced options
- Supported scanners:
  - Power Look series
  - Mirage series
  - Astra series
  - Vista series
  - UC series
  - others
  - Not listed scanners
  - UMAX scanner clones
- UMAX parallel port scanners
- Configuration
- Speed of UMAX scanners
- SANE-umax homepage
- SANE homepage
- XSane homepage

UMAX scanners
Astra series:
Name | SCSI-ID | Versions | UTA | ADF | B/W | Gray | Color | Bits/pixel | Resolution
Astra 600S | Astra 600S | all | UTA-2a |  | ok | ok | ok | 1,8,24 | 300 x 600
Astra 610S | Astra 610S | all | -- |  | ok | ok | ok | 1,8,24 | 300 x 600
Astra 1200S | Astra 1200S | all but 2.9 * | UTA-2a |  | ok | ok | ok | 1,8,10,24,30 | 600 x 1200
Astra 1220S | Astra 1220S | all | UTA-3a |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Astra 2100S | Astra 2100S | all | UTC-2100 |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Astra 2200 | Astra 2200 | all (2.1) ** | incl |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200
Astra 2400S | Astra 2400S | all (1.1) | UTA-2400 | X | ok | ok | ok | 1,8,12,24,36 | 600 x 2400
Astra 6400 | Astra 6400 | ? *** | X |  | ? | ? | ? | 1,8,14,24,42 | 600 x 1200
Astra 6450 | Astra 6450 | ? *** | incl |  | ? | ? | ? | 1,8,14,24,42 | 600 x 1200
Astra MX3 | Astra 2200 | ? ** | UTC-2100? |  | ok | ok | ok | 1,8,12,24,36 | 600 x 1200

* Astra 1200S-C with external power supply and Firmware Version 2.9 could make problems.
** Astra 2200 and MX3 are supported via SCSI. Connection via the USB bus not tested.
*** Astra 6400 and 6450 are firewire scanners: not tested.

UTA = Umax Transparancy Adapter, ADF = Automatic Document Feeder
(X = supported by scanner, incl = is included)

This page has been changed on 16th. december 2001

> Author: Oliver Rauch