sane-nec(5)

NAME
sane-nec - SANE backend for NEC scanners

DESCRIPTION
The sane-nec library implements a SANE (Scanner Access Now Easy) backend that provides access to NEC SCSI scanners. This backend should be considered alpha-quality software! In the current state it is known to work with PC-IN500/4C scanners. Another MultiReader scanner series is not supported. PC-IN 500/4C and MultiReader scanner are only sold in Japan.(except Multi Reader PetiScan.) For other scanners, it may or may not work.

The backend has the following known problems:
    - ColorLineart mode is not supported.
    - device name is fixed to /dev/scanner

At present, the following scanners are known to work with this backend.
    Vendor Product id
    ------ -----------
    NEC    PC-IN500/4C

FILES

/sane/etc/sane.d/nec.conf
    The backend configuration file.

/sane/lib/sane/libsane-nec.a
    The static library implementing this backend.

/sane/lib/sane/libsane-nec.so
    The shared library implementing this backend (present on systems that support dynamic loading).

ENVIRONMENT

SANE_DEBUG_NEC
    If the library was compiled with debug support enabled, this environment variable controls the debug level for this backend. E.g., a value of 128 requests all debug output to be printed. Smaller levels reduce verbosity.

SEE ALSO
sane(7), sane-scsi(5)

AUTHORS
Kazuya Fukuda