Compaq Support Software Diskette v4.60 For IBM OS/2

Versions and related updates of the OS/2 Drivers Supported
in this release

1.0 Storage Products

1.1 SCSI Adapters

1.1.1 CPQ53CX.ADD UPDATES - COMPAQ SCSI CONTROLLERS

CPQ53CX.ADD v2.0 - OS/2 SSD v1.11
* CPQ53CX.ADD v2.0 has replaced CPQC710.ADD for support of 32- Bit Fast-SCSI-2
controllers. CPQ53CX.ADD provides the same functionality as the CPQC710.ADD driver
as well as additional support. Additional functionality of CPQ53CX.ADD v2.0 is listed in
the following bullet. The install command files and readme file names have also changed
to ADD53CX.CMD, XPAND53C.BATand ADD53CX.RDM respectively.
* CPQ53CX.ADD v2.0 added support for the Compaq Insight Management Agents for
OS/2. This support allows monitoring of static SCSI configuration data. Dynamic run-time
SCSI data monitoring will be provided in a later release.

CPQ53CX.ADD v2.10 - OS/2 SSD v2.00
* CPQ53CX.ADD v2.10 has been updated to support the Integrated 32-Bit Fast-SCSI-2
Controller/P on the ProSignia 500 servers.
* CPQ53CX.ADD v2.10 has been updated to support the verbose command line option.
The /V option provides driver and controller information when the driver loads.
* CPQ53CX.ADD v2.10 has been updated to fix a TRAP E error during shutdown on
IBM OS/2 for SMP.
* CPQ53CX.ADD v2.10 has been updated to support the Compaq TurboDAT AutoLoader.
* CPQ53CX.ADD v2.10 has been updated to fix a boot problem with music CD-ROMs.
Prior to v2.10, the system would hang during boot if a music CD-ROM was in a CD-ROM
drive attached to a Fast-SCSI-2 controller.
* CPQ53CX.RDM has been incorporated into the \ADD\SCSI.RDM. SCSI.RDM contains
information on the 32-Bit Fast-SCSI-2 controller, the Systempro/XL Integrated SCSI-2
option port, the Deskpro XL Integrated PCI SCSI-2 controller, and the ProSignia 500
Integrated 32-Bit Fast-SCSI-2 Controller/P.
CPQ53CX.RDM, CPQC94.RDM, and ADDAMD.RDM have been removed.

CPQ53CX.ADD v2.11 - OS/2 SSD v2.01
* CPQ53CX.ADD v2.11 has been updated to incorporate support for the Compaq
ProLiant 1500 Integrated 32-Bit Fast-Wide SCSI-2 Controller/P, the Compaq
ProSignia 300 Integrated 32-Bit Fast- SCSI-2 Controller/P, the Compaq 32-Bit Fast-Wide
SCSI-2 Controller/P and the Compaq 32-Bit Fast-Wide SCSI-2 Controller/E.

CPQ53CX.ADD v2.12 - OS/2 SSD v2.02
* CPQ53CX.ADD v2.12 has been updated to incorporate run time SCSI statistics for
Compaq Insight Manager.

CPQ53CX.ADD v2.13 - OS/2 SSD v2.04
* CPQ53CX.ADD v2.13 has been updated to correct a potential problem running
5MB/Sec SCSI devices.

CPQ53CX.ADD v2.21 - OS/2 SSD v2.08
* CPQ53CX.ADD v2.21 has been updated to correct a potential problem running
SCSI devices on secondary PCI bus.

CPQ53CX.ADD v2.24 - OS/2 SSD v2.09
* CPQ53CX.ADD v2.24 has been updated to support the Compaq Wide-Ultra SCSI
Controllers.

CPQ53CX.ADD v2.26 - OS/2 SSD v2.10
* The SCSI driver, CPQ53CX.ADD v2.26 has been updated to correct a potential
problem of a system crash occurring while running a tape backup application and
the Compaq Insight Management Agent.

CPQ53CX.ADD v2.28 - OS/2 SSD v2.11
* The SCSI driver, CPQ53CX.ADD v2.28 has been updated to support
Ultra speeds (up to 40 MBps) on Ultra SCSI drives.

CPQ53CX.ADD v2.30 - OS/2 SSD v2.12
* The SCSI driver, CPQ53CX.ADD v2.30 has been updated to support pre-failure
reporting on S.M.A.R.T SCSI drives.

CPQ53CX.ADD v2.31 - OS/2 SSD v2.13
* The SCSI driver, CPQ53CX.ADD v2.31 has been updated to support the Integrated
Management Log on ProLiant 6000 and ProLiant 6500 servers.

CPQ53CX.ADD v2.40 - OS/2 SSD v2.15
* The SCSI driver, CPQ53CX.ADD v2.40 has been updated to support the Integrated
Dual Channel Wide-Ultra SCSI-3 Controller and the Integrate Management Log on
the Compaq ProLiant 3000 server.
* The SCSI driver, CPQ53CX.ADD v2.40 has been updated to support logging of
storage sub-system related power supply and fan redundancy failure events on
Compaq Servers that support the Integrated Management Log.
* The SCSI driver, CPQ53CX.ADD v2.40 can support up to 16 Compaq SCSI controllers
on a single Compaq server.

CPQ53CX.ADD v2.45 - OS/2 SSD v3.00
* The SCSI driver, CPQ53CX.ADD v2.45 has been updated to support Ultra speeds
(up to 40 MBps) on the Compaq ProLiant Storage System/U.

CPQ53CX.ADD v2.50 - OS/2 SSD v3.10
The Compaq SCSI driver, CPQ53CX.ADD Version 2.50 has been updated to fix
the following problem.
* The slowing down of the system when the CD storage System was switched off with
the Compaq Insight Manager Agents still running has been fixed.
* The system trap seen during a stress on 12X CD ROM Drive has been fixed.
This problem was observed only on ProLiant 5000 system.
* The driver has been fixed to support more than seven SCSI controllers on the system.

CPQ53CX.ADD v2.55 - OS/2 SSD v3.20
The Compaq SCSI driver, CPQ53CX.ADD Version 2.55 has
been enhanced to support controller redundancy. This enables the user to
configure two SCSI controllers as a duplex pair. Redundant/Secondary
controller takes over in case of primary controller failure.

CPQ53CX.ADD v2.60 - OS/2 SSD v3.30
The Compaq SCSI driver, CPQ53CX.ADD Version 2.60 has been enhanced to support
greater than 7 targets ids per bus.

CPQ53CX.ADD v2.70 - OS/2 SSD v3.40
The Compaq SCSI driver, CPQ53CX.ADD Version 2.70 has been enhanced to support
hot replace facility for Compaq SCSI Controllers. This version of the driver also
provides online pairing and dissolving of redundant back-up pairs of Compaq SCSI
Controllers.

CPQ53CX.ADD v2.75 - OS/2 SSD v3.50
The Compaq SCSI driver, CPQ53CX.ADD Version 2.75 has been enhanced to support
Compaq 64 bit Dual Channel Wide Ultra2 SCSI Controller.

CPQ53CX.ADD v2.76 - OS/2 SSD v3.55
The Compaq SCSI driver, CPQ53CX.ADD Version 2.76 has been enhanced to support
removeable media devices.

CPQ53CX.ADD v2.77 - OS/2 SSD v4.20
The Compaq SCSI driver, CPQ53CX.ADD Version 2.77 has been released
with bug fix for Agents .

CPQ53CX.ADD v2.78 - OS/2 SSD v4.30
The Compaq SCSI driver, CPQ53CX.ADD Version 2.78 has been enhanced to
support Compaq Dual Channel Wide Ultra 3-SCSI controller
with Raid On Chip capability.

CPQ53CX.ADD v2.79 - OS/2 SSD v4.40
The Compaq SCSI driver, CPQ53CX.ADD Version 2.79 has been released
with bug fix for Agents.

CPQ53CX.ADD v2.80 - OS/2 SSD v4.50
The Compaq SCSI driver, CPQ53CX.ADD Version 2.80 has been released
to support Compaq ProLiant ML350 Servers.

CPQ53CX.ADD v2.81 - OS/2 SSD v4.51
The Compaq SCSI driver, CPQ53CX.ADD Version 2.81 has been released
to fix an incorrect detail in the Resource Manager.

CPQ53CX.ADD v2.82 - OS/2 SSD v4.52
The Compaq SCSI driver, CPQ53CX.ADD Version 2.82 has been released
to enhance the support for 895A controller on Compaq Proliant ML330 Server.

CPQ53CX.ADD v2.83 - OS/2 SSD v4.59
The Compaq SCSI driver, CPQ53CX.ADD Version 2.83 has been released
to fix an Internal Processing error.

1.1.2 AICU160.ADD UPDATES - COMPAQ ADAPTEC SCSI CONTROLLERS

AICU160.ADD v10.1 - OS/2 SSD v4.50
The Compaq ADAPTEC SCSI driver, AICU160.ADD Version 10.1 has been enhanced
to support Adaptec Ultra-3 SCSI Controllers on Compaq Servers.

AICU160.ADD v10.2 - OS/2 SSD v4.51
The Compaq ADAPTEC SCSI driver, AICU160.ADD Version 10.2 has been enhanced
to support event logging and CIM support on Compaq Servers.

AICU160.ADD v10.21 - OS/2 SSD v4.55
The Compaq ADAPTEC SCSI driver, AICU160.ADD Version 10.21 has been updated
to fix the system hang problem that occurs if the BIOS32 driver, CPQB32.SYS
is present in the system.

1.1.3 OPTICAL.SYS - Removable Media Driver

OPTICAL.SYS v2.11 - OS/2 v2.08
* The Removable Media Driver which supports SCSI Removable peripherals
(i.e. PD-CD ROM Drive, Bernoulli Box, etc.).
OPTICAL.DDP v2.11 - OS/2 v2.08
* The Setup Profile Driver used with the OS/2 "Device Driver Install" utility
for installing the device driver OPTICAL.SYS.

1.2 Array Adapters

1.2.1 Compaq Array Driver Updates

CPQARRAY.ADD v2.00 - OS/2 SSD v2.00
* CPQARRAY.ADD v2.00 has been updated to incorporate performance improvements
in certain environments.
* CPQARRAY.ADD v2.00 has been updated to include command line options.
The /PERF option can be used to improve performance. The verbose /V option provides
driver and controller information when the driver loads. The /I option allows a controller
to be ignored by the driver. Refer to the CPQARRAY.RDM file for further information
about using these driver options.
* CPQARRAY.ADD v2.00 has been updated to support Insight Version Control.
* CPQARRAY.ADD v2.00 has been updated for SMART and IDA-2 controllers. Upon
shutdown, the driver will flush and disable the onboard battery backed-up cache.
This update preserves the controller battery life and ensures that data resident in the
controller cache is written to the attached disks.
* CPQARRAY.RDM v2.00 has been updated with command line option description.
The section on controller order has been clarified.

CPQARRAY.ADD v3.02 - OS/2 SSD v2.06
* CPQARRAY.ADD v3.02 has been updated to support the following new
Compaq Array Controllers:
Compaq SMART-2/E
Compaq SMART-2/P
CPQARRAY.ADD v3.05 - OS/2 SSD v2.08

* CPQARRAY.ADD v3.05 has been updated to correct a potential problem that
prevents the system from booting when the Array Accelerator is enabled on the
SMART-2 controller.
* CPQARRAY.ADD v3.05 has been updated to correct a potential problem that may
cause the system to lockup under heavy stress conditions.
CPQARRAY.ADD v3.06 - OS/2 SSD v2.09
* CPQARRAY.ADD v3.06 is a maintenance release that corrects an internal version
number mismatch with no functional or feature changes.

CPQARRAY.ADD v3.14 - OS/2 SSD v2.10
* The Array driver, CPQARRAY.ADD v 3.14 has been updated to provide support for
the Compaq Servers - ProLiant 800 and ProSignia 200.
* The Array driver, CPQARRAY.ADD v 3.14 has been updated to support the
Win-OS/2 Version of the Compaq Array Configuration utility on OS/2.
* The Array driver, CPQARRAY.ADD v 3.14 has been updated to correct a potential
system hang problem.
* The Array driver, CPQARRAY.ADD v 3.14 has been updated to correct a problem of
mismatch in controller slot / boot order on the ProLiant 2500.

CPQARRAY.ADD v3.15 - OS/2 SSD v2.12
* The Array driver, CPQARRAY.ADD v3.15 has been updated to support the Compaq
SMART-2SL controller.
* The Array driver, CPQARRAY.ADD v3.15 has been updated to support the
Integrated Management Log on the ProLiant 6000 Servers.
* The Array driver, CPQARRAY.ADD v3.15 has been updated to fix a 'Trap D' problem
which would occur during system boot when using a Compaq SMART Array controller.
This problem did not affect Compaq SMART-2 controllers.

CPQARRAY.ADD v3.16 - OS/2 SSD v2.13
* The Array driver, CPQARRAY.ADD v3.16 has been updated to support the
Integrated Management Log on the ProLiant 6000 and ProLiant 6500 Servers.

CPQARRAY.ADD v3.20 - OS/2 SSD v2.14
* The Array driver, CPQARRAY.ADD v3.20 has been updated to fix a problem with
SMART-2SL controller ordering.

CPQARRAY.ADD v3.25 - OS/2 SSD v2.15
* The Array driver, CPQARRAY.ADD v3.25 is a maintenance release with no changes
in functionality.

CPQARRAY.ADD v3.30 - OS/2 SSD v3.01
* The Array driver, CPQARRAY.ADD v3.30 has been updated to fix a potential hang
problem on Compaq servers that support the Integrated Management Log (IML).
* The Array driver, CPQARRAY.ADD V3.30 has been updated to support Compaq
Array Configuration Utility for Win-OS/2 Version 1.00.

CPQARRAY.ADD v3.40 - OS/2 SSD v3.10
* The Compaq Array Driver, CPQARRAY.ADD Version 3.40 has been enhanced
to support controller redundancy. This new feature enables the user to configure
two array controllers as redundant back-up pair using the command line option(/R).
The redundant controller takes over if the primary/active controller fails.
* The driver has been updated to fix hang/trap during system boot when an
interrupt(IRQ) is shared between two different types of controllers. This problem did
not affect the IRQ sharing between Array Controllers.

CPQARRAY.ADD v3.45 - OS/2 SSD v3.20
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version
3.45 has been updated to support the new Compaq SMART 3100ES Array Controller.

CPQARRAY.ADD v3.50 - OS/2 SSD v3.30
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version
3.50 has been updated to support the Compaq Smart Array 3200 Controller on OS/2.

CPQARRAY.ADD v3.60 - OS/2 SSD v3.40
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version
3.60 has been updated to provide hot replace facility for Compaq Array Controllers.
This version of the driver also provides online pairing and dissolving of redundant
back-up pairs of Compaq Array Controllers.

CPQARRAY.ADD v3.65 - OS/2 SSD v3.55
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.65
has been enhanced to support redundancy for SMART Array 3100ES Controllers.
The driver is updated to fix the Trap D problem when the CPQARRAY.ADD entry is
below IBM2FLPY.ADD in config.sys.

CPQARRAY.ADD v3.70 - OS/2 SSD v4.00
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.70
has been enhanced to support Compaq Smart Array 4200 Controllers.

CPQARRAY.ADD v3.71 - OS/2 SSD v4.10
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.71
has been enhanced to Compaq Smart Array 4250ES Controllers.

CPQARRAY.ADD v3.75 - OS/2 SSD v4.20
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.75
has been enhanced to support Hot replacement and FirmWare redundancy
for Compaq Smart Array 4250ES Controllers.

CPQARRAY.ADD v3.76 - OS/2 SSD v4.30
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.76
has been enhanced to support Compaq Smart Array 322DC Controllers and
Compaq Smart Array 431 Controllers.

CPQARRAY.ADD v3.77 - OS/2 SSD v4.50
* The Compaq Array Controller Driver for OS/2 CPQARRAY.ADD version 3.77
has been enhanced to support Compaq ProLiant ML350 Servers.

CPQARRAY.ADD v3.78 - OS/2 SSD v4.51
* The Compaq Array Controller Driver for OS/2, CPQARRAY.ADD version 3.78
has been enhanced to support Compaq RAID LC2 Controllers.

1.2.2 Compaq Fibre Channel Array Driver Updates

CPQFCAL.ADD v1.00 - OS/2 SSD v3.01
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.00 supports the
Compaq Fibre Channel Storage Systems on OS/2. The Compaq Fibre Channel Storage
System consists of Compaq Fibre Channel Host controller and Compaq Fibre Channel
Array controller connected on a Fibre Channel Arbitrated Loop (FCAL).
CPQFCAL.ADD v1.10 - OS/2 SSD v3.20
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.10 has
been enhanced to support controller redundancy. This enables the user
to configure two Fibre channel Array controllers as a duplex pair. Backup/secondary
controller takes over in case of primary controller failure.
CPQFCAL.ADD v1.15 - OS/2 SSD v3.30
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.15 has
been enhanced to support 12 port hub. This enables the user to connect
more storage systems (eleven) to a single Fibre Channel Host Array Controller.
CPQFCAL.ADD v1.20 - OS/2 SSD v3.40
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.20 has been
enhanced to support Hot replacement of Compaq Fibre Channel Array Controllers.
CPQFCAL.ADD v1.25 - OS/2 SSD v4.20
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.25 has been
enhanced to supports Online Making and Dissolving of Redundant
back-up pairs of Compaq Fibre Channel Array Controllers.
CPQFCAL.ADD v1.30 - OS/2 SSD v4.30
* The Compaq Fibre Channel driver for OS/2, CPQFCAL.ADD v1.30 has been
enhanced to support Compaq StorageWorks 64 Bit/66Mhz Fibre Channel Host Controllers.

1.2.3 Compaq CISS Driver Updates

CPQCISS.ADD v1.00 - OS/2 SSD 4.51
* The Compaq CISS Driver for OS/2, CPQCISS.ADD v1.00 supports Compaq Smart Array 5300 Controllers.

CPQCISS.ADD v1.10 - OS/2 SSD 4.52
* The Compaq CISS Driver for OS/2, CPQCISS.ADD v1.10 is enhanced to support SMB servers.

CPQCISS.ADD v1.20 - OS/2 SSD 4.53
* The Compaq CISS Driver for OS/2, CPQCISS.ADD v1.20 is enhanced to support Compaq Smart Array 532 Controller.

CPQCISS.ADD v1.30 - OS/2 SSD 4.59
* Added support for the following controllers
HP Smart Array 641 Controller
HP Smart Array 642 Controller

CPQCISS.ADD v1.32 - OS/2 SSD 4.60
* Fix for an internal processing error when issuing xcopy with verify option and lazy cache turned off.

1.3 EIDE Adapters

1.3.1 CPQEIDE.ADD - Compaq Integrated EIDE Controller

CPQEIDE.ADD v1.00 - OS/2 SSD 2.10
* The Compaq Bus Master IDE Driver for OS/2, CPQEIDE.ADD v 1.00 provides support
for the Compaq Enhanced IDE Controller on the Compaq Servers - ProLiant 2500,
ProLiant 800 and ProSignia 200.
* The Compaq Bus Master IDE Driver for OS/2, supports the Compaq Self-Monitoring
And Reporting Technology ( S.M.A.R.T ) drives. The Drive Failure Prediction is done
by the Compaq Insight Manager (CIM).

CPQEIDE.ADD v1.03 - OS/2 SSD 2.13
* The Compaq Bus Master IDE Driver for OS/2, CPQEIDE.ADD v 1.03 is a
maintenance release with no functional changes from v1.00.
The driver provides support for the Compaq Enhanced IDE Controller on the Compaq
Servers - ProLiant 6500, ProLiant 6000, ProLiant 2500, ProLiant 800, ProLiant 850R,
ProSignia 200 6/233 and ProSignia 200.

CPQEIDE.ADD v1.05 - OS/2 SSD 2.15
* The Compaq Bus Master IDE Driver for OS/2, CPQEIDE.ADD v1.05 has been
updated to support Maxtor 5.1GB IDE disk drives.

CPQEIDE.ADD v1.11- OS/2 SSD v3.00
* The Compaq Bus Master IDE Driver for OS/2, CPQEIDE.ADD v1.11 is a maintenance
release with no changes in functionality.

CPQEIDE.ADD v1.15- OS/2 SSD v3.01
* The Compaq EIDE driver for OS/2, CPQEIDE.ADD v1.15 has been updated to fix a
potential 'Trap D' that occurs on an OS/2 Warp system with more than 12 hard disk
drives and Fixpak 32 (XR_W032).
* The Compaq EIDE driver for OS/2, CPQEIDE.ADD v1.15 has been updated to
fix the below message appearing even if the IBM1S506.ADD entry does not exist
in CONFIG.SYS.
"CPQEIDE : Unable to allocate resources. Driver will be unloaded.
Please remove IBM1S506.ADD from CONFIG.SYS, if present."
* The Compaq EIDE driver for OS/2, CPQEIDE.ADD v1.15 has been updated to
fix a problem in reporting the Device Type to Compaq Insight Manager (CIM).

CPQEIDE.ADD v1.20 - OS/2 SSD v3.40
* The Compaq EIDE driver for OS/2, CPQEIDE.ADD v1.20 has been updated
to support IDE hard disks having the capacity greater than 8.5 GB.

2.0 Server Wellness Features

2.1 Compaq Server Wellness Support

CPQHLTH.EXE v2.10 - OS/2 SSD v1.11
* CPQHLTH.EXE v2.10 has been updated to support the Compaq Insight Management
Agents for OS/2 product.

CPQHLTH.EXE v2.20 - OS/2 SSD v2.00
* CPQHLTH.EXE v2.20 has been updated to support ProSignia 500 servers.
* CPQHLTH.EXE v2.20 has been updated to support Insight Version Control.

CPQHLTH.EXE v2.30 - OS/2 SSD v2.01
* CPQHLTH.EXE v2.30 has been updated to incorporate support for the Compaq
ProLiant 1500 and the Compaq ProSignia 300 Servers.

CPQHLTH.EXE v2.50 - OS/2 SSD v2.04
* CPQHLTH.EXE v2.50 has been updated to report EISA bus utilization via Compaq
Insight Manager.

CPQHLTH.EXE v2.64 - OS/2 SSD v2.13
* CPQHLTH.EXE v2.64 has been updated to provide support for the Compaq servers.
* ProLiant 6500 and ProLiant 6000.

CPQHLTH.EXE v2.70 - OS/2 SSD v2.14
The Health application, CPQHLTH.EXE v2.70 has been updated to support the Compaq
ProLiant 7000, ProLiant 1600 and ProLiant 1200 servers.

CPQHLTH.EXE v2.71 - OS/2 SSD v4.57
The Health application, CPQHLTH.EXE v2.71 has been updated to fix a system hang problem

2.2 Compaq Server System Management Driver

The Compaq System Management Driver contains support for G2 server onwards.
This driver will load only on these servers and unload on all the older machines. For G1 and
earlier servers, use SSD 4.56 available on the web. The driver supports the following features:
* Fan failure, and temperature monitoring.
* Power supply monitoring.
* Correctable Error Log.
* Critical Error Log.
* Automatic Server Recovery.

Compaq Server System Management Driver v3.0 - OS/2 SSD v4.57
* The Compaq Server System Management Driver Ver 3.0 for OS/2
supports Compaq ProLiant ML370 G2, Compaq ProLiant ML530 G2,
Compaq ProLiant ML350 G2, Compaq ProLiant ML350 G3, and
Compaq ProLiant ML370 G3 Servers.

Compaq Server System Management Driver v3.1 - OS/2 SSD v4.58
* The Compaq Server System Management Driver Ver3.1 for OS/2
has been enhanced to support Compaq ProLiant ML570(G2) Server.

2.3 Compaq BIOS-32 Helper Driver
Integrated Management Log Support

CPQB32.SYS v1.00 - OS/2 SSD v2.12
* The Compaq BIOS-32 Driver, CPQB32.SYS v1.00 is required for Integrated
Management Log support on the Compaq ProLiant 6000 servers.

CPQB32.SYS v2.00 - OS/2 SSD v2.13
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.00 is required for Integrated
Management Log (IML) support on the Compaq servers that Support IML.
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.00 has been updated to support the
Integrated Management Log with the Remote Insight Board.

CPQB32.SYS v2.05 - OS/2 SSD v3.01
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.05 has been updated to log IML
events related to System Fatal Fault (SFF).
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.05 has been enhanced to prevent a
NMI from getting generated when a PCI slot switch is toggled.

CPQB32.SYS v2.05 - OS/2 SSD v3.20
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.05 has been updated to log IML
events related to System Fatal Fault (SFF).
* The Compaq BIOS-32 Driver, CPQB32.SYS v2.05 has been enhanced to prevent an
NMI from getting generated when a PCI slot switch is toggled.

CPQB32.SYS v3.10 - OS/2 SSD v3.30
* The Compaq BIOS-32 Driver, CPQB32.SYS v3.10 has been updated for Hot Plug
and LCD support.

CPQB32.SYS v3.20 - OS/2 SSD v3.40
* The Compaq BIOS-32 Driver, CPQB32.SYS v3.20 is a maintenance release.

CPQB32.SYS v3.30 - OS/2 SSD v4.50
* The Compaq BIOS-32 Driver, CPQB32.SYS v3.30 has been updated to
support option ROM on SMB Servers.

CPQB32.SYS v3.31 - OS/2 SSD v4.51
* The Compaq Bios-32 Driver, CPQB32.SYS v3.31 has been updated to
fix an incorrect detail with Resource Manager.

CPQB32.SYS v3.32 - OS/2 SSD v4.58
* The Compaq Bios-32 Driver, CPQB32.SYS v3.32 has been updated to
fix the issue of the Adaptec driver, AICU160.ADD, not loading if CPQB32.SYS
has been loaded..

3.0 COMPAQ REMOTE INSIGHT SUPPORT
3.1 CPQRIB.SYS UPDATES

CPQRIB.SYS v1.00 - OS/2 SSD 2.08
* CPQRIB.SYS v1.00 provides support for the Compaq Remote Insight Controller.

CPQRIB.SYS v2.00 - OS/2 SSD 2.13
* CPQRIB.SYS v2.00 has been updated to support the Integrated Management Log
on ProLiant 6000 and ProLiant 6500.

CPQRIB.SYS v2.05 - OS/2 SSD 3.01
* CPQRIB.SYS v2.05 has been updated to fix the following problem:
Inability to manage the OS/2 server from Compaq Insight Manager (CIM) using a
Compaq Remote Insight Board with firmware Version 1.10 and Point-to-Point
Protocol (PPP).

CPQRIB.SYS v2.10 - OS/2 SSD 3.20
* CPQRIB.SYS v2.10 has been updated to fix the following problems.
* Hang problem when an event is logged in some systems with the RIB
driver CPQRIB.SYS, Health driver CPQHLTH.SYS and the BIOS-32 driver
CPQB32.SYS loaded and Compaq agents running on the system.
* Hang problem with the RIB driver CPQRIB.SYS loaded before the health driver
CPQHLTH.SYS in a configuration with the Compaq Remote Insight Board EISA card.
* The Trap-13 problem on boot.
* Also increased the IML buffer from 8K to 64K.

CPQRIB.SYS v2.15 - OS/2 SSD 3.30
* CPQRIB.SYS v2.15 has been updated to fix the following problems:
* IRQ Register to Resource Manager is made SHARED.
* Unlinking of the driver, if resource is not available is fixed.

CPQRIB.SYS v2.20 - OS/2 SSD 4.40
* CPQRIB.SYS v2.16 has been enhanced to support Remote Rom Flashing
on Remote Board Lights Out Edition of Controllers

4.0 PSD Updates for OS/2 SMP v2.11 and OS/2 Warp Server
Advanced 4.0 With SMP Support

4.1 OS2APIC.PSD Updates Compaq Platform Specific Driver For SMP Based OS/2

OS2APIC.PSD v1.10 - OS/2 SSD v2.05
* The OS2APIC.PSD v1.10 driver provided by Compaq supports ProLiant 1500 Servers
with the FlexSMP 5/133 Dual Processor Board.

OS2APIC.PSD v2.00 - OS/2 SSD v2.08
The OS2APIC.PSD v2.00 driver provided by Compaq supports the following systems:
* ProLiant 1500 Servers with the FlexSMP 5/133 Dual Processor Board.
* ProLiant 1500 Servers with the FlexSMP 5/166 Dual Processor Board.
* ProLiant 5000 Servers.

OS2APIC.PSD v2.10 - OS/2 SSD v2.09
The OS2APIC.PSD v2.10 driver provided by Compaq supports the following systems:
* Compaq ProLiant 1500 Servers with the FlexSMP 5/133 Dual Processor Board.
* Compaq ProLiant 1500 Servers with the FlexSMP 5/166 Dual Processor Board.
* Compaq ProLiant 5000 Servers.
* Compaq ProLiant 2500 Servers.

OS2APIC.PSD v2.20 - OS/2 SSD v2.10
The OS2APIC.PSD v2.20 driver provided by Compaq supports the following systems:
* Compaq ProLiant 1500 Servers with the FlexSMP 5/133 Dual Processor Board.
* Compaq ProLiant 1500 Servers with the FlexSMP 5/166 Dual Processor Board.
* Compaq ProLiant 5000 Servers.
* Compaq ProLiant 2500 Servers.
* Compaq ProLiant 800 Servers.

OS2APIC.PSD v2.30 - OS/2 SSD v2.12
The OS2APIC.PSD v2.30 driver provided by Compaq supports the following systems:
* Compaq ProLiant 7000 Servers.
* Compaq ProLiant 6500 Servers.
* Compaq ProLiant 6000 Servers.
* Compaq ProLiant 5500 Servers.
* Compaq ProLiant 1600 Servers.
* Compaq ProLiant 1500 Servers with the FlexSMP 5/133 Dual Processor Board.
* Compaq ProLiant 1500 Servers with the FlexSMP 5/166 Dual Processor Board.
* Compaq ProLiant 5000 Servers.
* Compaq ProLiant 3000 Servers.
* Compaq ProLiant 2500 Servers.
* Compaq ProLiant 800 and 850R Servers.

OS2APIC.PSD v2.40 - OS/2 SSD v3.00
The Compaq OS2APIC driver for OS/2, OS2APIC.PSD v2.40 has been updated to fix
a system hang problem during bootup with the Compaq ProLiant 7000 servers in a
4-Processor configuration.

OS2APIC.PSD v2.60 - OS/2 SSD v3.01
The Compaq OS2APIC driver for OS/2, OS2APIC.PSD v2.60 has been updated to
support additional command line options.

OS2APIC.PSD v2.61 - OS/2 SSD v3.10
* The Compaq OS2APIC driver for OS/2, OS2APIC.PSD v2.61 has been
updated to eliminate a minor bug observed with driver Version 2.60.

5.0 Compaq SSD Documentation For OS/2

Compaq SSD Documentation For OS/2 v1.00 - OS/2 SSD v3.10
The Compaq SSD Documentation from Compaq v1.00, is primarly used to read the HTM files
supplied with Support Software Diskette (SSD) for OS/2. It provides primary features like scroll
down/up, page up/down, Slider track Support, fileopen, Link support and Navigate back.

6.0 Miscellaneous Files

6.1 Obsolete Files - OS/2 SSD V4.54 and later

6.1.1 CPQACU - Compaq Array Configuration Utility

The Compaq Array Configuration Utility for OS/2 v2.21A has been enhanced to support
RAID/Stripe size migration, Online Logical Drive Exapansion and Redundant Controller
configuration of SMART Array 3100ES Controllers.

6.1.2 Compaq System Wellness Utility for OS/2

* Compaq System Wellness Utilities Version 2.21 has been updated to support
Compaq ProLiant 7000 Xeon 500 MHz.

6.1.3 Compaq SSD Setup Utility for OS/2

The Compaq SSD Setup Utility for OS/2 v1.2 has been updated to support Compaq Storage
Configuration utility. The Compaq SSD Setup Utility for OS/2 v1.2 requires Java Runtime
Environment v1.1.4 or above.

6.1.4 CPQSCU - Compaq Storage Configuration Utility

This utility is used for Hot replacement of Compaq Storage Controllers.
This utility supports SCSI, Array and Fibre Channel Controllers. It is
enhanced to support Compaq RAID LC2 controllers.

6.2 Obsolete Files - OS/2 SSD V3.20 and later

6.2.1 CPQWIZ.HTM - OS/2 SSD v3.20

* The reademe file CPQWIZ.HTM gives helpful installation instructions
to install compaq supplied drivers and Utilities.

6.3 Obsolete Files - OS/2 SSD V3.01 and later

6.3.1 CPQFCAL.RDM - OS/2 SSD v3.01
Compaq Fibre Channel Array Controller Driver Readme File

* The readme file CPQFCAL.RDM gives helpful installation instructions and
information about the CPQFCAL.ADD driver for OS/2 which supports the Compaq
Fibre Channel Controllers.

6.3.2 CPQACU.RDM - OS/2 SSD v3.01
Compaq Array Configuration Utility Readme File

* The readme file CPQFCAL.RDM gives helpful installation instructions and
information need to install the Compaq Array Configuration Utility.

6.3.3 PROLIANT.PSD

* The PROLIANT.PSD will not be available on OS/2 SSD v3.01 and later. This file is
required to support OS/2 SMP installations for multi-processor configurations on the
Compaq ProLiant 4500, 4000 and 2000 servers. For support of this products and
installation information, obtain a copy of OS/2 SSD v3.00.

6.3.4 PROLIANT.DDP

* The PROLIANT.DDP file will not be available on OS/2 SSD v3.01 and later. This is
the Device Driver Profile required to install PROLIANT.PSD using DDINSTAL.EXE.

6.3.5 VIDEO.RDM

* The file VIDEO.RDM will not be available on OS/2 SSD v3.01 and later.

6.3.6 AMSIO2.ADD

* The driver AMSIO2.ADD, that supports PC-SCSI and PCNet SCSI Controller on
Compaq Deskpro XL will not be available on the OS/2 SSD 3.01 and later. For support
of these products and installation information, obtain a copy of OS/2 SSD v3.00.

6.3.7 AMSIO2.EXE

* The Hardware detection program which determines the existence of PC-SCSI and
PCNet SCSI controllers will not be available on the OS/2 SSD v3.01 and later. For
support of these products and installation information obtain a copy of OS/2 SSD
v3.00

6.3.8 PC-SCSI.RDM

* The readme file PC-SCSI.RDM gives helpful installation instructions and
information about the AMSIO2 driver will not be available on OS/2 SSD v3.01 and later.

6.4 Obsolete Files - OS/2 SSD V3.00 and later

6.4.1 CQS_DATR.SYS

* Tape driver support under Sytos+ v1.0 will not be available on the OS/2 SSD 3.00
and later. For support of these products and installation information, obtain a copy
of OS/2 SSD v2.15. The following files are no longer on the OS/2 SSD:
\syfiles\cqs_datr.sys
\sysfiles\cqs_datr.dll
\sysfiles\cqs_datr.txt

6.4.2 CQS_1GBW.SYS

* 1.2GB ACA Tape support under Sytos+ will not be available on the OS/2 SSD 3.00
and later. For support of these products and installation information, obtain a copy of
OS/2 SSD v2.15. The following files are no longer on the OS/2 SSD:
\syfiles\cqs_1gbw.sys
\sysfiles\cqs_1gbw.dll
\sysfiles\cqs_1gbw.txt

6.4.3 CPQBZL.SYS

* Compaq Presario volume control button support driver will not be
available on the OS/2 SSD 3.00 and later. For support of these products and
installation information, obtain a copy of OS/2 SSD v2.15. The following files are
no longer on the OS/2 SSD:
\cpqbzl\cpqbzl.sys
\sysfiles\cpqbzl.rdm

6.4.4 CPQC94.ADD

The following files will not be available on the OS/2 SSD 3.00 and later.
For support of these products and installation information, obtain a copy
of OS/2 SSD v2.15.
\add\cpqc94.add
\sysfiles\cpqc94.rdm

6.5 Obsolete Files - OS/2 SSD V2.12 and later

6.5.1 CPQB32.RDM

CPQB32.RDM - OS/2 SSD 2.12
* A new file, CPQB32.RDM, has been added to the Compaq OS/2 Support Software
Diskette. This file provides the installation notes and lists the features of the Compaq
BIOS-32 driver (CPQB32.SYS).

6.6 Obsolete Files - OS/2 SSD V2.11 and later

6.6.1 OPTICAL.SYS - Removable Media Driver

OPTICAL.SYS v2.11 and OPTICAL.DDP v2.11 will not be available from
OS/2 SSD v3.30 and later.

6.7 Obsolete Files - OS/2 SSD V2.10 and later

6.7.1 EIDE.RDM

EIDE.RDM - OS/2 SSD v2.10
* A new file, EIDE.RDM, has been added to the Compaq OS/2 Support Software
diskette. This file:
- lists the controllers supported by the CPQEIDE.ADD driver
- provides the installation and troubleshooting instructions
- details the command line switches provided by the CPQEIDE.ADD driver

6.8 Obsolete Files - OS/2 SSD V2.00 and later

6.8.1 HISTORY.RDM

HISTORY.RDM - OS/2 SSD v2.00
* A new file, HISTORY.RDM, has been added to the Compaq OS/2 Support
Software diskette. This file contains a history of the changes made to the drivers and
support files shipped on the OS/2 SSD since v1.09. The latest changes will be found in
this file, WHATSNEW.RDM, and all previous changes will be found in HISTORY.RDM.
* README.1ST has been updated to reflect the removal of the OS/2 1.3 support.

-------------------------------------------------------------------------------------------------------------

Copyright 1998, 2005 Hewlett-Packard Development Company, L.P.
* OS/2 is a registered trademark of the IBM Corporation.
Other product names mentioned herein may be trademarks or registered
trademarks of their respective companies.