INTLBIOS.SYS v0.89 -- widescreen patch driver    2011-06-12    rlalla@stepnet.de
--------------------------------------------------------------------------------

Requirements:
 - Intel integrated graphics
 - Intel cpu with Intel 9xx or G3x/P3x or G4x/P4x or i3000 or i4500 chipset
   -or- Intel Core i3/i5/i7 cpu (1st or 2nd generation) 

Installation:
 - CONFIG.SYS: basedev=intlbios.sys /1680
    (or /0800 or /1024 or /1280 or /1360 or /1366 or /1400 or /1440 
     or /1600 or /HDTV or /1920)
 - Read startup message at reboot

What resolutions does it replace:
  /0800 : 1600x1200 -->  800x480
  /1024 : 1600x1200 --> 1024x600
  /1280 : 1600x1200 --> 1280x800
  /1360 : 1600x1200 --> 1360x768
  /1366 : 1600x1200 --> 1366x768
  /1400 : 1600x1200 --> 1400x1050
  /1440 : 1600x1200 --> 1440x900
  /1600 : 1600x1200 --> 1600x900
  /1680 : 1600x1200 --> 1680x1050 (default with no or wrong option)
  /HDTV : 1600x1200 --> 1920x1080 (option must be in capital characters)
  /1920 : 1600x1200 --> 1920x1200

Comment about 1366x768 resolution:
 - This mode is experimental. In case it does not work with your LCD TV, 
   you might try out 1360x768 instead.

Comment about 1920x1080 resolution:
 - This HDTV resolution mode is using "DVI reduced" horizontal timings.

Permanent restrictions:
 - Only resolutions smaller or equal to lcd resolution can be used.

Temporary restrictions:
 - Every computer manufacturer might arbitrarily modify the bios.
   In that case send me a copy of your bios to adapt the driver.

