ATOMBIOS.SYS v0.79 -- widescreen patch driver    2008-11-06    rlalla@stepnet.de
--------------------------------------------------------------------------------

Requirements:
 - ATI/AMD graphics chipset
 - ATOM-Bios (original pre-2008 style, or new DTD based style) 
 - Intel cpu with Intel 9xx or G3x/P3x or G4x/P4x memory controller
   -or- AMD64 cpu with any mainboard chipset

Installation:
 - CONFIG.SYS: basedev=atombios.sys
 - Read startup message at reboot

What resolutions does it replace:
 - EE: 1856x1392 --> 1280x800
 - EF: 1920x1440 --> 1440x900
 - EB: 1400x1050 --> 1680x1050

Permanent restrictions:
 - Only resolutions smaller or equal to lcd resolution can be used.

Temporary restrictions:
 - Every graphics card manufacturer might arbitrarily modify the bios.
   In that case send me a copy of your bios to adapt the driver to your card.
 - refresh rates are kept from original resolutions, except that 85Hz modes
   actually send now output at 60Hz for better support of analog lcd panels.
 - Intel cpu with non-Intel chipset or older AMD cpu are not supported.
   In case you need it, send me specs of the memory controller


