Server Systems Product Marketing

Option Description

Part # Supported Notes

Server Software:

SPARCserver 600MP - Unbundled Software Support Matrix

SPARCserver Manager No Migrate to Online: DiskSuite

SunDBE Database Excellerator v1.1 No New version (v1.2) due soon

Online: DiskSuite Yes

Backup CoPilot Yes

Online: Dual Port Tools Yes

Simplify SQL Yes

ARM and ASET Yes

PC-NFS Yes Requires v3.5

Local 3270 Yes Requires v7.0

X.25 Yes Requires v7.0

DNI Yes Requires v7.0

IR Yes Requires v6.0

SNA-3270 Yes Requires v6.1

Client-3270 Yes Requires v6.1

OSI Yes Requires v7.0

SNA Peer-to-Peer Yes Requires v6.0

CG3270 Yes Requires v7.0

SunNet License Yes

SunNet Manager Yes Requires v1.1

OpenWindows Yes v2.0 and v3.0

SunView Deskset Yes As part of OpenWindows 2.0

Sun GKS Yes Requires v4.0

Sun PHIGS Yes Requires v2.0

Sun XGL Yes Requires v2.0

X180A Sun Buttons No

X190A Sun Dials No

Windows:

Graphics:

Networking Software

Server Systems Product Marketing

Not tested, should work

No FB support

Tested and works on GX only

Not tested but should work

Tested and supported for upgrades

Tested and supported for upgrades

Option

Part # Supported Notes

SPARCserver 600MP - Options Compatibility Matrix

280 MB SMD Disk No

380 MB SMD Disk No

575 MB SMD Disk No

688 MB SMD Disk No

892 MB SMD Disk No

71 MB SCSI Disk No

140 MB SCSI Disk No

327 MB non-embedded SCSI Disk No

x559A 644 MB Sun CD CD-ROM Yes Internal or Desktop SunCD Pack

660_ 150 MB 1/4" SCSI Tape Drive Yes Internal or Desktop Tape Pack

680A Front-Load 1/2" Tape Drive Yes Tabletop, System or Exp Cabinet

60 MB (QIC-11/24) SCSI Tape No Migrate to 150 MB 1/4" Tape

1600 bpi 1/2" Tape Drive No Migrate to FLT

675A 6250 bpi 1/2" Tape Drive (non-FLT) No Migrate to FLT

19" Color (66/76Hz) Yes

16" Color (66/76Hz) No

21" Color (76Hz)

19" Analog (grayscale)

17" Analog (grayscale)

19" ECL mono Yes

19" hi-res mono Yes

327-MB embedded SCSI disk Yes Internal or External add-on

669-MB embedded SCSI disk Yes Internal or External add-on

1.3-GB embedded SCSI disk Yes Internal or External add-on

1.0-GB (3MB/S) IPI disk Yes

911-MB (6MB/S) IPI disk Yes

1.3-GB 5.25" IPI disk Yes Requires firmware update (x2080A)

130 MB SMD Disk No

Peripherals:

Monitors:

No

No

No

Server Systems Product Marketing

Use 1054A, SBE/S

Not supported or tested

Option Description

Part # Supported Notes

SPARCserver 600MP - Options Compatibility Matrix

1054A SCSI / Buffered Ethernet Card Yes

1021A Sun SBus Prestoserve Yes

1008A Serial Parallel Interface Yes Requires v1.1 driver

x1009A Sun Net High Speed Serial Interface Yes

x1004 Sun Net Token Ring Interconnect Yes Requires v1.2 driver (avail. later)

SPRN-400 SPARCPrinter SBus Printer Card Yes

X450A SBus Ethernet Card No Use 1054A, SBE/S

408A ISP-80 IPI Disk Controller Yes New 1.3GB disks require new firmware

(firmware update pn X2080A)

165A Sun VME Prestoserve Yes Accelerates IPI disk only. Need v2.3

driver. For SCSI use SBus Prestoserve.

HSI SunNet High-Speed Serial Interface No Use SBus HSI/S (x1009A)

461A SunNet FDDI/DX Yes Requires v2.0 software (FDA-2.0-...)

482_ ALM-2 16-channel Asynch Line Multi Yes Maximum of 8 in 16�slot cabinet

MCP SunNet Multi Protocol Comm.Proc. Yes Supported on Upgraded Systems

CHA SunLink Channel Gateway Yes Requires v7.1 software update

NC400 Interphase NC400 Network CoProc. Yes Requires software revision

XY472 1/2" Tape Controller No Migrate to FLT

XY450/451 SMD Disk Controller No Migrate to SCSI or IPI

x410A SMD-4 Disk Ctlr (also x401A) No Migrate to SCSI or IPI

Multibus 2nd Ethernet Controller No Migrate to 1054A

3/E 2nd Ethernet Controller No Migrate to 1054A

x598A Sun-3 SCSI Host Adapter No Migrate to 1054A

452A SunNet Ethernet VME Controller No Migrate to 1054A

CG3 / CG5 No Replace with SBus GX

SBus Cards:

VME Boards:

X1055A SBus SCSI Host Adapter No

X218A VideoPix No Not tested

CXP / GXP No Not supported or tested

TAAC No

VX / MVX No

Sun Video ? Check with Parallax

Not supported or tested