T0 TIGA System Installation 
Di1
^top
z
|
|You have to install the TIGA system files into C:\TIGA directory. OK ?
|
=2Y
@2Y/N: 
e %2 y ^inst
j ^insend
^inst
z
f c:\tiga\tigacd.exe ^notiga
|
|You already have a directory C:\TIGA where AUTOINS will install TIGA
|system files into. AUTOINS will overwrite your old TIGA system files.
j ^waitkey
^notiga
|
|You don't have a directory C:\TIGA where AUTOINS will install TIGA
|system files into. AUTOINS will make the directory C:\TIGA to install.
^waitkey
!Hit any key to continue.
z
|
|Installing...  TIGA system from Drive %1 to C:\TIGA
|
f %1\TIGA\TIGACD.EXE ^errend
c %1\TIGA\*.* c:\tiga\ ^errend
=2C:\UTIL
z
|
|Type the target drive and directory to copy the utility programs to.
@2Target Drive and Directory : 
e "%2" "" ^inst
e %2 esc ^inst
z
|
|Installing...  TIGA utility programs from Drive %1 to %2
|
c %1\UTIL\*.* %2\ ^errend
z
|
|In order for TIGA system to be installed, AUTOINS needs to modify your
|AUTOEXEC.BAT and CONFIG.SYS files.
|
|Do you want AUTOINS modify your AUTOEXEC.BAT and CONFIG.SYS files ? 
=2Y
@2Y/N: 
e %2 y ^autochange
z
|
|You have to modify your AUTOEXEC.BAT and CONFIG.SYS files later.
|
|Do you need the sample files as AUTOEXEC.TIG and CONFIG.TIG ? 
=2Y
@2Y/N: 
z
|
e %2 y ^selfchange
j ^nochange
^selfchange
c c:\config.sys c:\config.tig
c c:\autoexec.bat c:\autoexec.tig
m c:\config.tig %1\sys\sr340.sys ^srerr
#%1\modtext c:\autoexec.tig PATH= PATH_= 0
#%1\modtext c:\autoexec.tig PATH= PATH_ 0
#%1\modtext c:\autoexec.tig PATH=C:\TIGA; PATH= 1
#%1\modtext c:\autoexec.tig SET_TIGA=-mC:\TIGA_-lC:\TIGA_-i0x60 SET_TIGA=
#%1\modtext c:\autoexec.tig TIGACD
z
|
|The AUTOEXEC.TIG and CONFIG.TIG files which are made in the directory C:\
|will help you modify your AUTOEXEC.BAT and CONFIG.SYS files.
^nochange
|TIGA system installation is completed. Refer to the TIGA installation
|manual for detail.
b
^autochange
m c:\config.sys %1\sys\sr340.sys ^srerr
#%1\modtext c:\autoexec.bat PATH= PATH_= 0
#%1\modtext c:\autoexec.bat PATH= PATH_ 0
#%1\modtext c:\autoexec.bat PATH=C:\TIGA; PATH= 1
#%1\modtext c:\autoexec.bat SET_TIGA=-mC:\TIGA_-lC:\TIGA_-i0x60 SET_TIGA=
#%1\modtext c:\autoexec.bat TIGACD
z
|
|TIGA system installation is completed and your CONFIG.SYS and AUTOEXEC.BAT
|files have been modified corresponding to the TIGA system. After you reboot
|your system, TIGA menu will appear. Then, select an appropriate video mode
|from the available list. Refer to the TIGA installation manual for detail.
b
^srerr
|
|Unable to install SR340.SYS.
j ^errend
^auerr
|
|Unable to open/create AUTOEXEC.BAT.
j ^errend
^errend
|
|Error occurred.
|Please reinstall.
b
^insend
z
|
|Prepare your system before installing the TIGA system.
b
