InS_StArT
E100ISA.COM
1.1
^Intel EtherExpress(TM) PRO/100 ISA Adapter,E100ISA.COM,IE0000,E100ISA
?This is the DOSODI driver for Intel EtherExpress(TM) PRO/100 ISA Adapter.
!OIE0000(MEDIATYPE)Optional Media Type Setting
?Note: Media Type should be requested if the LAN is Full Duplex.
@AUTO
HALF10
FULL10
HALF100
FULL100
!OIE0000(RXEARLY)Optional PipeLining Request
?Note: RXEARLY can increase driver performance but is not supported under Windows95 or with Client32.
@OFF
ON
!OIE0000(USE32BITIO)Optional 32 Bit Access Enable
?Note: USE32BITIO can increase driver performance but is not supported by some motherboard chipsets.
@NO
YES
$OIE0000(NODE ADDRESS)Node Address
0
FFFFFFFFFFFF
$OIE0000(SERIAL)Optional Serial Number
?Note: SERIAL is only required if multiple @dName adapters are installed.  
0
FFFFFF
*RIE0000(FRAME)Frame Type
?Note: Ethernet_802.2 is the default frame type for ODI drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD

