InS_StArT
E100SODI.COM
1.1
^Intel EtherExpress(TM) PRO/100 Smart Adapter,E100SODI.COM,0000P0
?This is the DOSODI client driver for the Intel EtherExpress(TM) PRO/100 Smart Adapter.
$00000P0(SLOT) Optional PCI Slot Number
?This option is only required for multiple adapter installations.  See the documentation for your PCI system for valid slot numbers.
1
99999
!00000P0(SPEED) Optional Line Speed
10
100
*0IEMAP0(FRAME) Frame Type
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$0IEMAP0(NODE ADDRESS) Optional Adapter Node Address
?CAUTION:  This number must be unique.  An invalid number can cause serious network problems.  The second digit must be 2, 6, A, or E.
020000000000
FEFFFFFFFFFF
InS_EnD

