The Amateur Radio Project - Multiples and sub-multiples, abbreviations and indices

# Multiples and sub-multiples, abbreviations and indices

### Question 10 of 12

A current of 3mA flows through a resistor when a p.d. of 12V is connected across its terminals. The resistor has a resistance value of

1. 0.25
2. 4
3. 250
4. 4 k

1 | 2 | 3 | 4

Back

page (tq0210)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details