The Amateur Radio Project - Measurements

# Measurements

### Question 30 of 32

A frequency meter has a quoted tolerance of 10 parts per 100,000. When measuring a signal at exactly 14MHz, it will have a reading between

1. 13.9986MHz and 14MHz
2. 13.9986MHz and 14.0014MHz
3. 13.9993MHz and 14.0007MHz
4. 14MHz and 14.0014MHz

1 | 2 | 3 | 4

Back |

page (tq2330)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details