The Amateur Radio Project - Simple alternating current circuits

# Simple alternating current circuits

### Question 13 of 14

A 4 F capacitor is connected in series with an 8F capacitor. The combination is connected across a 12V AC supply. The p.d. across the 4 F and 8 F capacitor respectively will be

1. 4V, 8V
2. 6V, 6V
3. 8V, 4V
4. 9V, 3V

1 | 2 | 3 | 4

Back |

page (tq0813)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details