# Propagation

### Explanation of question 24

The ratio maximum usable frequency / critical frequency is

1. less than unity
2. unity
3. two
4. greater than unity

The answer is :- 4 The maximum usable frequency (m.u.f.) is greater than the critical frequency. The ratio will therefore be greater than unity.

BACK

page (tq2124ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details