The Amateur Radio Project - Transmitter interference

# Transmitter interference

### Question 12 of 17

The risk of mains-borne interference may be reduced by using

1. the house mains earth to dissipate any RF
2. an earth leakage trip
3. an external high-resistance RF earth
4. an external low-resistance RF earth

1 | 2 | 3 | 4

Back |

page (tq2412)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd | Contact details