# Licensing conditions

### Explanation of question 24

A VHF antenna should be situated

1. as near as possible to any domestic radio receiving antenna
2. at least 20m above any other receiving antenna
3. at least 50m from any other receiving antenna
4. as far as possible from any other receiving antenna

The answer is :- 4

BACK

page (tq2624ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details