# Transmitter interference

### Explanation of question 3

‘Chirp’ is caused by

1. inadequate harmonic suppression
2. overmodulation
3. the loading effect of keying
4. a defect in the speech amplifier

The answer is :- 3 Poor frequency stability of the oscillator, caused by loading as the key is closed, is the prime cause of chirp.

BACK

page (tq2403ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details