# F.M., A.M. and S.S.B. transmitters

### Explanation of question 16

An SSB transmitter would have its carrier suppressed by a

1. sideband generator
2. product detector
3. balanced modulator
4. diode detector

The answer is :- 3 Carrier suppression is achieved by a balanced modulator. The word ‘balanced’ refers to the balancing of its bridge circuit.

BACK

page (tq1816ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details