# Oscillators

### Explanation of question 5

In Fig. 16.1, the ratio C4 to C5 predominantly determines the

1. resonant frequency
2. amount of feedback
3. gain
4. time constant

The answer is :- 2 Variation of the C. to C5 ratio will determine the amount of feedback. Often, these have the same value and are ganged together.

BACK

page (tq1605ex)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details