The Amateur Radio Project - Multiples and sub-multiples, abbreviations and indices

# Multiples and sub-multiples, abbreviations and indices

### Question 12 of 12

A 12k resistor has a p.d. of 24mV applied across its terminals. The current through the resistor will be

1. 0.5mA
2. 0.5 A
3. 2 mA
4. 2 A

1 | 2 | 3 | 4

Back

page (tq0212)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details