The Amateur Radio Project - Propagation

# Propagation

### Question 22 of 30

Critical frequency is defined as

1. the highest frequency returned to earth when radiation is vertically upwards
2. the maximum frequency reflected by the ionosphere
3. that frequency at the end of a particular frequency band
4. the lowest frequency that will radiate from an antenna

1 | 2 | 3 | 4

Back |

page (tq2122)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details