The Amateur Radio Project - Practical resistors

# Practical resistors

### Question 1 of 6

A 1.2 resistor has a tolerance of 10%. Its resistance value will lie between

1. 1.2k and 1.32k
2. 1.14k and 1.26k
3. 1.08k and 1.32k
4. 1.08k and 1.20k

1 | 2 | 3 | 4

Back |

page (tq0401)
Some material Copyright John Bowyer G4KGS.
Click here for important Copyright information
Web Space provided by Hostroute.com Ltd
Contact details